{"text_format":"1","workbook":"xlsx","n_sheets":8,"sheets":["Poznámky","HrubýVstup","KG_BT","KT_BT","BytovéTesty","KG_Adresáře","KT_Adresáře","TestManipulaceSAdresáři"],"not_rendered":{"charts":4,"images":0,"macros":1,"external_links":0,"defined_names":5,"comments":3,"pivot_tables":2},"unopened":[{"sheet":"KG_BT","index":2,"reason":"not_a_worksheet"},{"sheet":"KG_Adresáře","index":5,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Poznámky","index":0,"n_rows":5,"n_cols":6,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[null,null,"Počet Filesystémů","Počet karet","Počet disků"]
[null,null,4,7,3,{"$f":"PRODUCT(C5:E5)","v":84}]

{"sheet":"HrubýVstup","index":1,"n_rows":523,"n_cols":18,"rows_kept":523,"cut":false,"hidden":false,"merged":[]}
["MKSoft DiskSpeed 4.2  Copyright © 1989-92 MKSoft Development",null,null,null,null,"File Create in files/sec","CPU Available","File Open in files/sec","CPU Available","Directory Scan in files/sec","CPU Available","File Delete in files/sec","CPU Available","Seek/Read (seeks/sec)","CPU Available","CPU Speed Rating","Average CPU Available","CPU Availability Index"]
["------------------------------------------------------------",null,null,null,"Test1",{"$f":"VALUE(MID(HrubýVstup!$A$10,23,3))","v":569},{"$f":"VALUE(RIGHT(HrubýVstup!$A$10,3))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(RIGHT(LEFT($A$11,26),5))","v":774},{"$f":"VALUE(RIGHT(HrubýVstup!$A$11,3))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(RIGHT(LEFT($A$12,26),5))","v":3019},{"$f":"VALUE(RIGHT(HrubýVstup!$A$12,3))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(RIGHT(LEFT($A$13,26),5))","v":804},{"$f":"VALUE(RIGHT(HrubýVstup!$A$13,3))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(RIGHT(LEFT($A$15,26),5))","v":1273},{"$f":"VALUE(RIGHT(HrubýVstup!$A$15,3))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(RIGHT(HrubýVstup!$A$7,HrubýVstup!$B$7))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(MID(HrubýVstup!$A$137,24,3))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(RIGHT(HrubýVstup!$A$137,HrubýVstup!$B$8))","v":{"$error":"#VALUE!"}}]
["CPU: 68040  AmigaOS Version: 40.68  Normal Video DMA",null,null,null,"Test2",{"$f":"VALUE(MID(HrubýVstup!$A$149,23,3))","v":568},{"$f":"VALUE(RIGHT(HrubýVstup!$A$149,3))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(RIGHT(LEFT($A$150,26),5))","v":770},{"$f":"VALUE(RIGHT(HrubýVstup!$A$150,3))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(RIGHT(LEFT($A$151,26),5))","v":3027},{"$f":"VALUE(RIGHT(HrubýVstup!$A$151,3))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(RIGHT(LEFT($A$152,26),5))","v":789},{"$f":"VALUE(RIGHT(HrubýVstup!$A$152,3))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(RIGHT(LEFT($A$154,26),5))","v":1277},{"$f":"VALUE(RIGHT(HrubýVstup!$A$154,3))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(RIGHT(HrubýVstup!$A$146,HrubýVstup!$B$7))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(MID(HrubýVstup!$A$276,24,3))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(RIGHT(HrubýVstup!$A$276,HrubýVstup!$B$8))","v":{"$error":"#VALUE!"}}]
["Device:  dh0:    Buffers: 300",null,null,null,"Test3",{"$f":"VALUE(MID(HrubýVstup!$A$288,23,3))","v":564},{"$f":"VALUE(RIGHT(HrubýVstup!$A$288,3))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(RIGHT(LEFT($A$289,26),5))","v":771},{"$f":"VALUE(RIGHT(HrubýVstup!$A$289,3))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(RIGHT(LEFT($A$290,26),5))","v":3026},{"$f":"VALUE(RIGHT(HrubýVstup!$A$290,3))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(RIGHT(LEFT($A$291,26),5))","v":790},{"$f":"VALUE(RIGHT(HrubýVstup!$A$291,3))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(RIGHT(LEFT($A$293,26),5))","v":1277},{"$f":"VALUE(RIGHT(HrubýVstup!$A$293,3))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(RIGHT(HrubýVstup!$A$285,HrubýVstup!$B$7))","v":{"$error":"#VALUE!"}},{"$f":"VALUE(MID(HrubýVstup!$A$415,24,3))","v":0.09},{"$f":"VALUE(RIGHT(HrubýVstup!$A$415,HrubýVstup!$B$8))","v":444}]
["Comments: PFS3_68060_CF_Blizzard1260_128MBRAM_1"]
[null,"Počet číslic",null,null,null,"Kontrola"]
["CPU Calibration shows that CPU availability tests",4,null,null,null,null,{"$f":"P1","v":"CPU Speed Rating"},"Average CPU Available","CPU Availability Index"]
[null,4,null,null,"Test1",{"$f":"$A$137","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Testing directory manipulation speed.",null,null,null,"Test2",{"$f":"$A$276","v":0},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["File Create:          569 files/sec",null,null,null,"Test3",{"$f":"$A$415","v":"Average CPU Available: 9%  |  CPU Availability index: 444"},{"$error":"#VALUE!"},0.09,444]
["File Open:            774 files/sec"]
["Directory Scan:      3019 files/sec",null,null,null,null,{"$f":"523-415","v":108}]
["File Delete:          804 files/sec"]
[]
["Seek/Read:           1273 seeks/sec"]
[null,null,null,null,"Pomocný","Type of test","Size (bytes)","Tested Memory","Aligned buffer","Pomocný","Create file in bytes/sec","CPU Available","Pomocný","Write to file in bytes/sec","CPU Available","Pomocný","Read from file in bytes/sec","CPU Available"]
["Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",null,null,null,null,{"$f":"A17","v":"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer."},{"$f":"VALUE(MID(F17,16,3))","v":512},{"$f":"MID(F17,26,9)","v":"MEMF_FAST"},{"$f":"MID(F17,37,4)","v":"LONG"},null,{"$f":"VALUE(RIGHT(LEFT(A18,26),9))","v":669120},{"$f":"VALUE(RIGHT(A18,3))","v":{"$error":"#VALUE!"}},null,{"$f":"VALUE(RIGHT(LEFT(A19,26),9))","v":534784},{"$f":"VALUE(RIGHT(A19,3))","v":{"$error":"#VALUE!"}},null,{"$f":"VALUE(RIGHT(LEFT(A20,26),9))","v":350484},{"$f":"VALUE(RIGHT(A20,3))","v":{"$error":"#VALUE!"}}]
["Create file:       669120 bytes/sec",null,null,null,{"$f":"ADDRESS(ROW()-1+5,1)","v":"$A$22"},{"$f":"INDIRECT(E18)","v":"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer."},{"$f":"VALUE(MID(F18,16,4))","v":4096},{"$f":"MID(F18,27,9)","v":"MEMF_FAST"},{"$f":"MID(F18,38,4)","v":"LONG"},{"$f":"ADDRESS(ROW()+5,1)","v":"$A$23"},{"$f":"VALUE(RIGHT(LEFT(INDIRECT(J18),26),9))","v":915456},{"$f":"VALUE(RIGHT(INDIRECT(J18),3))","v":{"$error":"#VALUE!"}},{"$f":"ADDRESS(ROW()+1+5,1)","v":"$A$24"},{"$f":"VALUE(RIGHT(LEFT(INDIRECT(M18),26),9))","v":648704},{"$f":"VALUE(RIGHT(INDIRECT(M18),3))","v":{"$error":"#VALUE!"}},{"$f":"ADDRESS(ROW()+2+5,1)","v":"$A$25"},{"$f":"VALUE(RIGHT(LEFT(INDIRECT(P18),26),9))","v":1309696},{"$f":"VALUE(RIGHT(INDIRECT(P18),3))","v":{"$error":"#VALUE!"}}]
["Write to file:     534784 bytes/sec",null,null,null,{"$f":"IF(LEN(E18)=5,ADDRESS(RIGHT(E18,2)+5,1),ADDRESS(RIGHT(E18,3)+5,1))","v":"$A$27"},"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",{"$f":"VALUE(MID(F19,16,5))","v":32768},{"$f":"MID(F19,28,9)","v":"MEMF_FAST"},{"$f":"MID(F19,39,4)","v":"LONG"},{"$f":"IF(LEN(J18)=5,ADDRESS(RIGHT(J18,2)+5,1),ADDRESS(RIGHT(J18,3)+5,1))","v":"$A$28"},{"$f":"VALUE(RIGHT(LEFT(INDIRECT(J19),26),9))","v":1656808},{"$f":"VALUE(RIGHT(INDIRECT(J19),3))","v":{"$error":"#VALUE!"}},{"$f":"IF(LEN(M18)=5,ADDRESS(RIGHT(M18,2)+5,1),ADDRESS(RIGHT(M18,3)+5,1))","v":"$A$29"},{"$f":"VALUE(RIGHT(LEFT(INDIRECT(M19),26),9))","v":1534082},{"$f":"VALUE(RIGHT(INDIRECT(M19),3))","v":{"$error":"#VALUE!"}},{"$f":"IF(LEN(P18)=5,ADDRESS(RIGHT(P18,2)+5,1),ADDRESS(RIGHT(P18,3)+5,1))","v":"$A$30"},{"$f":"VALUE(RIGHT(LEFT(INDIRECT(P19),26),9))","v":1955443},{"$f":"VALUE(RIGHT(INDIRECT(P19),3))","v":{"$error":"#VALUE!"}}]
["Read from file:    350484 bytes/sec",null,null,null,{"$f":"IF(LEN(E19)=5,ADDRESS(RIGHT(E19,2)+5,1),ADDRESS(RIGHT(E19,3)+5,1))","v":"$A$32"},"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",{"$f":"VALUE(MID(F20,16,6))","v":262144},{"$f":"MID(F20,29,9)","v":"MEMF_FAST"},{"$f":"MID(F20,40,4)","v":"LONG"},{"$f":"IF(LEN(J19)=5,ADDRESS(RIGHT(J19,2)+5,1),ADDRESS(RIGHT(J19,3)+5,1))","v":"$A$33"},1830431,{"$error":"#VALUE!"},{"$f":"IF(LEN(M19)=5,ADDRESS(RIGHT(M19,2)+5,1),ADDRESS(RIGHT(M19,3)+5,1))","v":"$A$34"},1680824,{"$error":"#VALUE!"},{"$f":"IF(LEN(P19)=5,ADDRESS(RIGHT(P19,2)+5,1),ADDRESS(RIGHT(P19,3)+5,1))","v":"$A$35"},2111444,{"$error":"#VALUE!"}]
[null,null,null,null,"$A$37","Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",{"$f":"VALUE(MID(F21,16,3))","v":512},{"$f":"MID(F21,26,9)","v":"MEMF_FAST"},{"$f":"MID(F21,37,4)","v":"WORD"},"$A$38",617723,{"$error":"#VALUE!"},"$A$39",653888,{"$error":"#VALUE!"},"$A$40",336277,{"$error":"#VALUE!"}]
["Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",null,null,null,"$A$42","Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",{"$f":"VALUE(MID(F22,16,4))","v":4096},{"$f":"MID(F22,27,9)","v":"MEMF_FAST"},{"$f":"MID(F22,38,4)","v":"WORD"},"$A$43",888320,{"$error":"#VALUE!"},"$A$44",878592,{"$error":"#VALUE!"},"$A$45",1176064,{"$error":"#VALUE!"}]
["Create file:       915456 bytes/sec",null,null,null,"$A$47","Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",{"$f":"VALUE(MID(F23,16,5))","v":32768},{"$f":"MID(F23,28,9)","v":"MEMF_FAST"},{"$f":"MID(F23,39,4)","v":"WORD"},"$A$48",1468628,{"$error":"#VALUE!"},"$A$49",1340137,{"$error":"#VALUE!"},"$A$50",1685445,{"$error":"#VALUE!"}]
["Write to file:     648704 bytes/sec",null,null,null,"$A$52","Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",{"$f":"VALUE(MID(F24,16,6))","v":262144},{"$f":"MID(F24,29,9)","v":"MEMF_FAST"},{"$f":"MID(F24,40,4)","v":"WORD"},"$A$53",1434618,{"$error":"#VALUE!"},"$A$54",1465401,{"$error":"#VALUE!"},"$A$55",1810118,{"$error":"#VALUE!"}]
["Read from file:   1309696 bytes/sec",null,null,null,"$A$57","Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",{"$f":"VALUE(MID(F25,16,3))","v":512},{"$f":"MID(F25,26,9)","v":"MEMF_FAST"},{"$f":"MID(F25,37,4)","v":"BYTE"},"$A$58",624000,{"$error":"#VALUE!"},"$A$59",625856,{"$error":"#VALUE!"},"$A$60",336448,{"$error":"#VALUE!"}]
[null,null,null,null,"$A$62","Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",{"$f":"VALUE(MID(F26,16,4))","v":4096},{"$f":"MID(F26,27,9)","v":"MEMF_FAST"},{"$f":"MID(F26,38,4)","v":"BYTE"},"$A$63",911872,{"$error":"#VALUE!"},"$A$64",861696,{"$error":"#VALUE!"},"$A$65",1174016,{"$error":"#VALUE!"}]
["Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",null,null,null,"$A$67","Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",{"$f":"VALUE(MID(F27,16,5))","v":32768},{"$f":"MID(F27,28,9)","v":"MEMF_FAST"},{"$f":"MID(F27,39,4)","v":"BYTE"},"$A$68",1482752,{"$error":"#VALUE!"},"$A$69",1276356,{"$error":"#VALUE!"},"$A$70",1687552,{"$error":"#VALUE!"}]
["Create file:      1656808 bytes/sec",null,null,null,"$A$72","Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",{"$f":"VALUE(MID(F28,16,6))","v":262144},{"$f":"MID(F28,29,9)","v":"MEMF_FAST"},{"$f":"MID(F28,40,4)","v":"BYTE"},"$A$73",1576080,{"$error":"#VALUE!"},"$A$74",1497965,{"$error":"#VALUE!"},"$A$75",1810118,{"$error":"#VALUE!"}]
["Write to file:    1534082 bytes/sec",null,null,null,"$A$77","Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",{"$f":"VALUE(MID(F29,16,3))","v":512},{"$f":"MID(F29,26,9)","v":"MEMF_CHIP"},{"$f":"MID(F29,37,4)","v":"LONG"},"$A$78",579584,{"$error":"#VALUE!"},"$A$79",493138,{"$error":"#VALUE!"},"$A$80",328086,{"$error":"#VALUE!"}]
["Read from file:   1955443 bytes/sec",null,null,null,"$A$82","Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",{"$f":"VALUE(MID(F30,16,4))","v":4096},{"$f":"MID(F30,27,9)","v":"MEMF_CHIP"},{"$f":"MID(F30,38,4)","v":"LONG"},"$A$83",737280,{"$error":"#VALUE!"},"$A$84",767488,{"$error":"#VALUE!"},"$A$85",829440,{"$error":"#VALUE!"}]
[null,null,null,null,"$A$87","Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",{"$f":"VALUE(MID(F31,16,5))","v":32768},{"$f":"MID(F31,28,9)","v":"MEMF_CHIP"},{"$f":"MID(F31,39,4)","v":"LONG"},"$A$88",903543,{"$error":"#VALUE!"},"$A$89",923387,{"$error":"#VALUE!"},"$A$90",1092266,{"$error":"#VALUE!"}]
["Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",null,null,null,"$A$92","Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",{"$f":"VALUE(MID(F32,16,6))","v":262144},{"$f":"MID(F32,29,9)","v":"MEMF_CHIP"},{"$f":"MID(F32,40,4)","v":"LONG"},"$A$93",1052402,{"$error":"#VALUE!"},"$A$94",1044658,{"$error":"#VALUE!"},"$A$95",1135524,{"$error":"#VALUE!"}]
["Create file:      1830431 bytes/sec",null,null,null,"$A$97","Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",{"$f":"VALUE(MID(F33,16,3))","v":512},{"$f":"MID(F33,26,9)","v":"MEMF_CHIP"},{"$f":"MID(F33,37,4)","v":"WORD"},"$A$98",500736,{"$error":"#VALUE!"},"$A$99",507520,{"$error":"#VALUE!"},"$A$100",296602,{"$error":"#VALUE!"}]
["Write to file:    1680824 bytes/sec",null,null,null,"$A$102","Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",{"$f":"VALUE(MID(F34,16,4))","v":4096},{"$f":"MID(F34,27,9)","v":"MEMF_CHIP"},{"$f":"MID(F34,38,4)","v":"WORD"},"$A$103",670720,{"$error":"#VALUE!"},"$A$104",642269,{"$error":"#VALUE!"},"$A$105",827904,{"$error":"#VALUE!"}]
["Read from file:   2111444 bytes/sec",null,null,null,"$A$107","Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",{"$f":"VALUE(MID(F35,16,5))","v":32768},{"$f":"MID(F35,28,9)","v":"MEMF_CHIP"},{"$f":"MID(F35,39,4)","v":"WORD"},"$A$108",918156,{"$error":"#VALUE!"},"$A$109",618187,{"$error":"#VALUE!"},"$A$110",1043176,{"$error":"#VALUE!"}]
[null,null,null,null,"$A$112","Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",{"$f":"VALUE(MID(F36,16,6))","v":262144},{"$f":"MID(F36,29,9)","v":"MEMF_CHIP"},{"$f":"MID(F36,40,4)","v":"WORD"},"$A$113",961408,{"$error":"#VALUE!"},"$A$114",902832,{"$error":"#VALUE!"},"$A$115",1090929,{"$error":"#VALUE!"}]
["Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",null,null,null,{"$f":"IF(LEN(E36)=5,ADDRESS(RIGHT(E36,2)+5,1),ADDRESS(RIGHT(E36,3)+5,1))","v":"$A$117"},"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",{"$f":"VALUE(MID(F37,16,3))","v":512},{"$f":"MID(F37,26,9)","v":"MEMF_CHIP"},{"$f":"MID(F37,37,4)","v":"BYTE"},"$A$118",453383,{"$error":"#VALUE!"},"$A$119",396096,{"$error":"#VALUE!"},"$A$120",279389,{"$error":"#VALUE!"}]
["Create file:       617723 bytes/sec",null,null,null,"$A$122","Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",{"$f":"VALUE(MID(F38,16,4))","v":4096},{"$f":"MID(F38,27,9)","v":"MEMF_CHIP"},{"$f":"MID(F38,38,4)","v":"BYTE"},"$A$123",571190,{"$error":"#VALUE!"},"$A$124",568832,{"$error":"#VALUE!"},"$A$125",702609,{"$error":"#VALUE!"}]
["Write to file:     653888 bytes/sec",null,null,null,"$A$127","Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",{"$f":"VALUE(MID(F39,16,5))","v":32768},{"$f":"MID(F39,28,9)","v":"MEMF_CHIP"},{"$f":"MID(F39,39,4)","v":"BYTE"},"$A$128",741763,{"$error":"#VALUE!"},"$A$129",707723,{"$error":"#VALUE!"},"$A$130",852865,{"$error":"#VALUE!"}]
["Read from file:    336277 bytes/sec",null,null,null,"$A$132","Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",{"$f":"VALUE(MID(F40,16,6))","v":262144},{"$f":"MID(F40,29,9)","v":"MEMF_CHIP"},{"$f":"MID(F40,40,4)","v":"BYTE"},"$A$133",786746,{"$error":"#VALUE!"},"$A$134",757094,{"$error":"#VALUE!"},"$A$135",885407,{"$error":"#VALUE!"}]
[]
["Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer."]
["Create file:       888320 bytes/sec"]
["Write to file:     878592 bytes/sec"]
["Read from file:   1176064 bytes/sec"]
[]
["Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer."]
["Create file:      1468628 bytes/sec"]
["Write to file:    1340137 bytes/sec"]
["Read from file:   1685445 bytes/sec"]
[]
["Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer."]
["Create file:      1434618 bytes/sec"]
["Write to file:    1465401 bytes/sec"]
["Read from file:   1810118 bytes/sec"]
[]
["Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer."]
["Create file:       624000 bytes/sec"]
["Write to file:     625856 bytes/sec"]
["Read from file:    336448 bytes/sec"]
[]
["Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer."]
["Create file:       911872 bytes/sec"]
["Write to file:     861696 bytes/sec"]
["Read from file:   1174016 bytes/sec"]
[]
["Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer."]
["Create file:      1482752 bytes/sec"]
["Write to file:    1276356 bytes/sec"]
["Read from file:   1687552 bytes/sec"]
[]
["Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer."]
["Create file:      1576080 bytes/sec"]
["Write to file:    1497965 bytes/sec"]
["Read from file:   1810118 bytes/sec"]
[]
["Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.","CHIP RAM"]
["Create file:       579584 bytes/sec"]
["Write to file:     493138 bytes/sec"]
["Read from file:    328086 bytes/sec"]
[]
["Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer."]
["Create file:       737280 bytes/sec"]
["Write to file:     767488 bytes/sec"]
["Read from file:    829440 bytes/sec"]
[]
["Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer."]
["Create file:       903543 bytes/sec"]
["Write to file:     923387 bytes/sec"]
["Read from file:   1092266 bytes/sec"]
[]
["Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer."]
["Create file:      1052402 bytes/sec"]
["Write to file:    1044658 bytes/sec"]
["Read from file:   1135524 bytes/sec"]
[]
["Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer."]
["Create file:       500736 bytes/sec"]
["Write to file:     507520 bytes/sec"]
["Read from file:    296602 bytes/sec"]
[]
["Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer."]
["Create file:       670720 bytes/sec"]
["Write to file:     642269 bytes/sec"]
["Read from file:    827904 bytes/sec"]
[]
["Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer."]
["Create file:       918156 bytes/sec"]
["Write to file:     618187 bytes/sec"]
["Read from file:   1043176 bytes/sec"]
[]
["Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer."]
["Create file:       961408 bytes/sec"]
["Write to file:     902832 bytes/sec"]
["Read from file:   1090929 bytes/sec"]
[]
["Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer."]
["Create file:       453383 bytes/sec"]
["Write to file:     396096 bytes/sec"]
["Read from file:    279389 bytes/sec"]
[]
["Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer."]
["Create file:       571190 bytes/sec"]
["Write to file:     568832 bytes/sec"]
["Read from file:    702609 bytes/sec"]
[]
["Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer."]
["Create file:       741763 bytes/sec"]
["Write to file:     707723 bytes/sec"]
["Read from file:    852865 bytes/sec"]
[]
["Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer."]
["Create file:       786746 bytes/sec"]
["Write to file:     757094 bytes/sec"]
["Read from file:    885407 bytes/sec"]
[]
[]
["MKSoft DiskSpeed 4.2  Copyright © 1989-92 MKSoft Development"]
["------------------------------------------------------------"]
["CPU: 68040  AmigaOS Version: 40.68  Normal Video DMA"]
["Device:  dh0:    Buffers: 300"]
["Comments: PFS3_68060_CF_Blizzard1260_128MBRAM_2"]
[]
[]
[]
["No CPU Speed Rating -- CPU % not available."]
[]
["Testing directory manipulation speed."]
["File Create:          568 files/sec"]
["File Open:            770 files/sec"]
["Directory Scan:      3027 files/sec"]
["File Delete:          789 files/sec"]
[]
["Seek/Read:           1277 seeks/sec"]
[null,null,null,null,"Pomocný","Type of test","Size (bytes)","Tested Memory","Aligned buffer","Pomocný","Create file in bytes/sec","CPU Available","Pomocný","Write to file in bytes/sec","CPU Available","Pomocný","Read from file in bytes/sec","CPU Available"]
["Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",null,null,null,null,{"$f":"A156","v":"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer."},{"$f":"VALUE(MID(F156,16,3))","v":512},{"$f":"MID(F156,26,9)","v":"MEMF_FAST"},{"$f":"MID(F156,37,4)","v":"LONG"},null,{"$f":"VALUE(RIGHT(LEFT(A157,26),9))","v":667456},{"$f":"VALUE(RIGHT(A157,3))","v":{"$error":"#VALUE!"}},null,{"$f":"VALUE(RIGHT(LEFT(A158,26),9))","v":544576},{"$f":"VALUE(RIGHT(A158,3))","v":{"$error":"#VALUE!"}},null,{"$f":"VALUE(RIGHT(LEFT(A159,26),9))","v":350740},{"$f":"VALUE(RIGHT(A159,3))","v":{"$error":"#VALUE!"}}]
["Create file:       667456 bytes/sec",null,null,null,{"$f":"ADDRESS(ROW()-1+5,1)","v":"$A$161"},{"$f":"INDIRECT(E157)","v":"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer."},{"$f":"VALUE(MID(F157,16,4))","v":4096},{"$f":"MID(F157,27,9)","v":"MEMF_FAST"},{"$f":"MID(F157,38,4)","v":"LONG"},{"$f":"ADDRESS(ROW()+5,1)","v":"$A$162"},{"$f":"VALUE(RIGHT(LEFT(INDIRECT(J157),26),9))","v":896000},{"$f":"VALUE(RIGHT(INDIRECT(J157),3))","v":{"$error":"#VALUE!"}},{"$f":"ADDRESS(ROW()+1+5,1)","v":"$A$163"},{"$f":"VALUE(RIGHT(LEFT(INDIRECT(M157),26),9))","v":660480},{"$f":"VALUE(RIGHT(INDIRECT(M157),3))","v":{"$error":"#VALUE!"}},{"$f":"ADDRESS(ROW()+2+5,1)","v":"$A$164"},{"$f":"VALUE(RIGHT(LEFT(INDIRECT(P157),26),9))","v":1311232},{"$f":"VALUE(RIGHT(INDIRECT(P157),3))","v":{"$error":"#VALUE!"}}]
["Write to file:     544576 bytes/sec",null,null,null,{"$f":"IF(LEN(E157)=5,ADDRESS(RIGHT(E157,2)+5,1),ADDRESS(RIGHT(E157,3)+5,1))","v":"$A$166"},"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",{"$f":"VALUE(MID(F158,16,5))","v":32768},{"$f":"MID(F158,28,9)","v":"MEMF_FAST"},{"$f":"MID(F158,39,4)","v":"LONG"},{"$f":"IF(LEN(J157)=5,ADDRESS(RIGHT(J157,2)+5,1),ADDRESS(RIGHT(J157,3)+5,1))","v":"$A$167"},{"$f":"VALUE(RIGHT(LEFT(INDIRECT(J158),26),9))","v":1695744},{"$f":"VALUE(RIGHT(INDIRECT(J158),3))","v":{"$error":"#VALUE!"}},{"$f":"IF(LEN(M157)=5,ADDRESS(RIGHT(M157,2)+5,1),ADDRESS(RIGHT(M157,3)+5,1))","v":"$A$168"},{"$f":"VALUE(RIGHT(LEFT(INDIRECT(M158),26),9))","v":998176},{"$f":"VALUE(RIGHT(INDIRECT(M158),3))","v":{"$error":"#VALUE!"}},{"$f":"IF(LEN(P157)=5,ADDRESS(RIGHT(P157,2)+5,1),ADDRESS(RIGHT(P157,3)+5,1))","v":"$A$169"},{"$f":"VALUE(RIGHT(LEFT(INDIRECT(P158),26),9))","v":1959534},{"$f":"VALUE(RIGHT(INDIRECT(P158),3))","v":{"$error":"#VALUE!"}}]
["Read from file:    350740 bytes/sec",null,null,null,{"$f":"IF(LEN(E158)=5,ADDRESS(RIGHT(E158,2)+5,1),ADDRESS(RIGHT(E158,3)+5,1))","v":"$A$171"},"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",{"$f":"VALUE(MID(F159,16,6))","v":262144},{"$f":"MID(F159,29,9)","v":"MEMF_FAST"},{"$f":"MID(F159,40,4)","v":"LONG"},{"$f":"IF(LEN(J158)=5,ADDRESS(RIGHT(J158,2)+5,1),ADDRESS(RIGHT(J158,3)+5,1))","v":"$A$172"},1695458,{"$error":"#VALUE!"},{"$f":"IF(LEN(M158)=5,ADDRESS(RIGHT(M158,2)+5,1),ADDRESS(RIGHT(M158,3)+5,1))","v":"$A$173"},1708933,{"$error":"#VALUE!"},{"$f":"IF(LEN(P158)=5,ADDRESS(RIGHT(P158,2)+5,1),ADDRESS(RIGHT(P158,3)+5,1))","v":"$A$174"},2111444,{"$error":"#VALUE!"}]
[null,null,null,null,"$A$176","Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",{"$f":"VALUE(MID(F160,16,3))","v":512},{"$f":"MID(F160,26,9)","v":"MEMF_FAST"},{"$f":"MID(F160,37,4)","v":"WORD"},"$A$177",633000,{"$error":"#VALUE!"},"$A$178",659136,{"$error":"#VALUE!"},"$A$179",336192,{"$error":"#VALUE!"}]
["Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",null,null,null,"$A$181","Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",{"$f":"VALUE(MID(F161,16,4))","v":4096},{"$f":"MID(F161,27,9)","v":"MEMF_FAST"},{"$f":"MID(F161,38,4)","v":"WORD"},"$A$182",888832,{"$error":"#VALUE!"},"$A$183",876032,{"$error":"#VALUE!"},"$A$184",1174016,{"$error":"#VALUE!"}]
["Create file:       896000 bytes/sec",null,null,null,"$A$186","Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",{"$f":"VALUE(MID(F162,16,5))","v":32768},{"$f":"MID(F162,28,9)","v":"MEMF_FAST"},{"$f":"MID(F162,39,4)","v":"WORD"},"$A$187",1454539,{"$error":"#VALUE!"},"$A$188",1349030,{"$error":"#VALUE!"},"$A$189",1685445,{"$error":"#VALUE!"}]
["Write to file:     660480 bytes/sec",null,null,null,"$A$191","Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",{"$f":"VALUE(MID(F163,16,6))","v":262144},{"$f":"MID(F163,29,9)","v":"MEMF_FAST"},{"$f":"MID(F163,40,4)","v":"WORD"},"$A$192",1439992,{"$error":"#VALUE!"},"$A$193",1454559,{"$error":"#VALUE!"},"$A$194",1810118,{"$error":"#VALUE!"}]
["Read from file:   1311232 bytes/sec",null,null,null,"$A$196","Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",{"$f":"VALUE(MID(F164,16,3))","v":512},{"$f":"MID(F164,26,9)","v":"MEMF_FAST"},{"$f":"MID(F164,37,4)","v":"BYTE"},"$A$197",619776,{"$error":"#VALUE!"},"$A$198",631274,{"$error":"#VALUE!"},"$A$199",337109,{"$error":"#VALUE!"}]
[null,null,null,null,"$A$201","Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",{"$f":"VALUE(MID(F165,16,4))","v":4096},{"$f":"MID(F165,27,9)","v":"MEMF_FAST"},{"$f":"MID(F165,38,4)","v":"BYTE"},"$A$202",911872,{"$error":"#VALUE!"},"$A$203",855552,{"$error":"#VALUE!"},"$A$204",1174016,{"$error":"#VALUE!"}]
["Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",null,null,null,"$A$206","Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",{"$f":"VALUE(MID(F166,16,5))","v":32768},{"$f":"MID(F166,28,9)","v":"MEMF_FAST"},{"$f":"MID(F166,39,4)","v":"BYTE"},"$A$207",1470464,{"$error":"#VALUE!"},"$A$208",1347584,{"$error":"#VALUE!"},"$A$209",1685445,{"$error":"#VALUE!"}]
["Create file:      1695744 bytes/sec",null,null,null,"$A$211","Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",{"$f":"VALUE(MID(F167,16,6))","v":262144},{"$f":"MID(F167,29,9)","v":"MEMF_FAST"},{"$f":"MID(F167,40,4)","v":"BYTE"},"$A$212",1597643,{"$error":"#VALUE!"},"$A$213",927094,{"$error":"#VALUE!"},"$A$214",1810118,{"$error":"#VALUE!"}]
["Write to file:     998176 bytes/sec",null,null,null,"$A$216","Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",{"$f":"VALUE(MID(F168,16,3))","v":512},{"$f":"MID(F168,26,9)","v":"MEMF_CHIP"},{"$f":"MID(F168,37,4)","v":"LONG"},"$A$217",588352,{"$error":"#VALUE!"},"$A$218",592960,{"$error":"#VALUE!"},"$A$219",327191,{"$error":"#VALUE!"}]
["Read from file:   1959534 bytes/sec",null,null,null,"$A$221","Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",{"$f":"VALUE(MID(F169,16,4))","v":4096},{"$f":"MID(F169,27,9)","v":"MEMF_CHIP"},{"$f":"MID(F169,38,4)","v":"LONG"},"$A$222",786944,{"$error":"#VALUE!"},"$A$223",756224,{"$error":"#VALUE!"},"$A$224",828928,{"$error":"#VALUE!"}]
[null,null,null,null,"$A$226","Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",{"$f":"VALUE(MID(F170,16,5))","v":32768},{"$f":"MID(F170,28,9)","v":"MEMF_CHIP"},{"$f":"MID(F170,39,4)","v":"LONG"},"$A$227",944627,{"$error":"#VALUE!"},"$A$228",964245,{"$error":"#VALUE!"},"$A$229",1090904,{"$error":"#VALUE!"}]
["Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",null,null,null,"$A$231","Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",{"$f":"VALUE(MID(F171,16,6))","v":262144},{"$f":"MID(F171,29,9)","v":"MEMF_CHIP"},{"$f":"MID(F171,40,4)","v":"LONG"},"$A$232",1070637,{"$error":"#VALUE!"},"$A$233",1020511,{"$error":"#VALUE!"},"$A$234",1135524,{"$error":"#VALUE!"}]
["Create file:      1695458 bytes/sec",null,null,null,"$A$236","Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",{"$f":"VALUE(MID(F172,16,3))","v":512},{"$f":"MID(F172,26,9)","v":"MEMF_CHIP"},{"$f":"MID(F172,37,4)","v":"WORD"},"$A$237",506304,{"$error":"#VALUE!"},"$A$238",513728,{"$error":"#VALUE!"},"$A$239",297397,{"$error":"#VALUE!"}]
["Write to file:    1708933 bytes/sec",null,null,null,"$A$241","Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",{"$f":"VALUE(MID(F173,16,4))","v":4096},{"$f":"MID(F173,27,9)","v":"MEMF_CHIP"},{"$f":"MID(F173,38,4)","v":"WORD"},"$A$242",657408,{"$error":"#VALUE!"},"$A$243",517044,{"$error":"#VALUE!"},"$A$244",829952,{"$error":"#VALUE!"}]
["Read from file:   2111444 bytes/sec",null,null,null,"$A$246","Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",{"$f":"VALUE(MID(F174,16,5))","v":32768},{"$f":"MID(F174,28,9)","v":"MEMF_CHIP"},{"$f":"MID(F174,39,4)","v":"WORD"},"$A$247",918156,{"$error":"#VALUE!"},"$A$248",820220,{"$error":"#VALUE!"},"$A$249",1041875,{"$error":"#VALUE!"}]
[null,null,null,null,"$A$251","Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",{"$f":"VALUE(MID(F175,16,6))","v":262144},{"$f":"MID(F175,29,9)","v":"MEMF_CHIP"},{"$f":"MID(F175,40,4)","v":"WORD"},"$A$252",953250,{"$error":"#VALUE!"},"$A$253",900617,{"$error":"#VALUE!"},"$A$254",1090929,{"$error":"#VALUE!"}]
["Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",null,null,null,{"$f":"IF(LEN(E175)=5,ADDRESS(RIGHT(E175,2)+5,1),ADDRESS(RIGHT(E175,3)+5,1))","v":"$A$256"},"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",{"$f":"VALUE(MID(F176,16,3))","v":512},{"$f":"MID(F176,26,9)","v":"MEMF_CHIP"},{"$f":"MID(F176,37,4)","v":"BYTE"},"$A$257",445312,{"$error":"#VALUE!"},"$A$258",440181,{"$error":"#VALUE!"},"$A$259",279069,{"$error":"#VALUE!"}]
["Create file:       633000 bytes/sec",null,null,null,"$A$261","Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",{"$f":"VALUE(MID(F177,16,4))","v":4096},{"$f":"MID(F177,27,9)","v":"MEMF_CHIP"},{"$f":"MID(F177,38,4)","v":"BYTE"},"$A$262",574976,{"$error":"#VALUE!"},"$A$263",561474,{"$error":"#VALUE!"},"$A$264",703121,{"$error":"#VALUE!"}]
["Write to file:     659136 bytes/sec",null,null,null,"$A$266","Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",{"$f":"VALUE(MID(F178,16,5))","v":32768},{"$f":"MID(F178,28,9)","v":"MEMF_CHIP"},{"$f":"MID(F178,39,4)","v":"BYTE"},"$A$267",762141,{"$error":"#VALUE!"},"$A$268",719996,{"$error":"#VALUE!"},"$A$269",852865,{"$error":"#VALUE!"}]
["Read from file:    336192 bytes/sec",null,null,null,"$A$271","Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",{"$f":"VALUE(MID(F179,16,6))","v":262144},{"$f":"MID(F179,29,9)","v":"MEMF_CHIP"},{"$f":"MID(F179,40,4)","v":"BYTE"},"$A$272",793414,{"$error":"#VALUE!"},"$A$273",567820,{"$error":"#VALUE!"},"$A$274",885407,{"$error":"#VALUE!"}]
[]
["Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer."]
["Create file:       888832 bytes/sec"]
["Write to file:     876032 bytes/sec"]
["Read from file:   1174016 bytes/sec"]
[]
["Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer."]
["Create file:      1454539 bytes/sec"]
["Write to file:    1349030 bytes/sec"]
["Read from file:   1685445 bytes/sec"]
[]
["Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer."]
["Create file:      1439992 bytes/sec"]
["Write to file:    1454559 bytes/sec"]
["Read from file:   1810118 bytes/sec"]
[]
["Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer."]
["Create file:       619776 bytes/sec"]
["Write to file:     631274 bytes/sec"]
["Read from file:    337109 bytes/sec"]
[]
["Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer."]
["Create file:       911872 bytes/sec"]
["Write to file:     855552 bytes/sec"]
["Read from file:   1174016 bytes/sec"]
[]
["Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer."]
["Create file:      1470464 bytes/sec"]
["Write to file:    1347584 bytes/sec"]
["Read from file:   1685445 bytes/sec"]
[]
["Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer."]
["Create file:      1597643 bytes/sec"]
["Write to file:     927094 bytes/sec"]
["Read from file:   1810118 bytes/sec"]
[]
["Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.","CHIP RAM"]
["Create file:       588352 bytes/sec"]
["Write to file:     592960 bytes/sec"]
["Read from file:    327191 bytes/sec"]
[]
["Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer."]
["Create file:       786944 bytes/sec"]
["Write to file:     756224 bytes/sec"]
["Read from file:    828928 bytes/sec"]
[]
["Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer."]
["Create file:       944627 bytes/sec"]
["Write to file:     964245 bytes/sec"]
["Read from file:   1090904 bytes/sec"]
[]
["Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer."]
["Create file:      1070637 bytes/sec"]
["Write to file:    1020511 bytes/sec"]
["Read from file:   1135524 bytes/sec"]
[]
["Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer."]
["Create file:       506304 bytes/sec"]
["Write to file:     513728 bytes/sec"]
["Read from file:    297397 bytes/sec"]
[]
["Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer."]
["Create file:       657408 bytes/sec"]
["Write to file:     517044 bytes/sec"]
["Read from file:    829952 bytes/sec"]
[]
["Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer."]
["Create file:       918156 bytes/sec"]
["Write to file:     820220 bytes/sec"]
["Read from file:   1041875 bytes/sec"]
[]
["Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer."]
["Create file:       953250 bytes/sec"]
["Write to file:     900617 bytes/sec"]
["Read from file:   1090929 bytes/sec"]
[]
["Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer."]
["Create file:       445312 bytes/sec"]
["Write to file:     440181 bytes/sec"]
["Read from file:    279069 bytes/sec"]
[]
["Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer."]
["Create file:       574976 bytes/sec"]
["Write to file:     561474 bytes/sec"]
["Read from file:    703121 bytes/sec"]
[]
["Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer."]
["Create file:       762141 bytes/sec"]
["Write to file:     719996 bytes/sec"]
["Read from file:    852865 bytes/sec"]
[]
["Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer."]
["Create file:       793414 bytes/sec"]
["Write to file:     567820 bytes/sec"]
["Read from file:    885407 bytes/sec"]
[]
[]
[]
[]
["MKSoft DiskSpeed 4.2  Copyright © 1989-92 MKSoft Development"]
["------------------------------------------------------------"]
["CPU: 68040  AmigaOS Version: 40.68  Normal Video DMA"]
["Device:  dh0:    Buffers: 300"]
["Comments: PFS3_68060_CF_Blizzard1260_128MBRAM_3"]
[]
["No CPU Speed Rating -- CPU % not available."]
[]
["Testing directory manipulation speed."]
["File Create:          564 files/sec"]
["File Open:            771 files/sec"]
["Directory Scan:      3026 files/sec"]
["File Delete:          790 files/sec"]
[]
["Seek/Read:           1277 seeks/sec"]
[null,null,null,null,"Pomocný","Type of test","Size (bytes)","Tested Memory","Aligned buffer","Pomocný","Create file in bytes/sec","CPU Available","Pomocný","Write to file in bytes/sec","CPU Available","Pomocný","Read from file in bytes/sec","CPU Available"]
["Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",null,null,null,null,{"$f":"A295","v":"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer."},{"$f":"VALUE(MID(F295,16,3))","v":512},{"$f":"MID(F295,26,9)","v":"MEMF_FAST"},{"$f":"MID(F295,37,4)","v":"LONG"},null,{"$f":"VALUE(RIGHT(LEFT(A296,26),9))","v":676224},{"$f":"VALUE(RIGHT(A296,3))","v":{"$error":"#VALUE!"}},null,{"$f":"VALUE(RIGHT(LEFT(A297,26),9))","v":690688},{"$f":"VALUE(RIGHT(A297,3))","v":{"$error":"#VALUE!"}},null,{"$f":"VALUE(RIGHT(LEFT(A298,26),9))","v":348436},{"$f":"VALUE(RIGHT(A298,3))","v":{"$error":"#VALUE!"}}]
["Create file:       676224 bytes/sec",null,null,null,{"$f":"ADDRESS(ROW()-1+5,1)","v":"$A$300"},{"$f":"INDIRECT(E296)","v":"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer."},{"$f":"VALUE(MID(F296,16,4))","v":4096},{"$f":"MID(F296,27,9)","v":"MEMF_FAST"},{"$f":"MID(F296,38,4)","v":"LONG"},{"$f":"ADDRESS(ROW()+5,1)","v":"$A$301"},{"$f":"VALUE(RIGHT(LEFT(INDIRECT(J296),26),9))","v":911360},{"$f":"VALUE(RIGHT(INDIRECT(J296),3))","v":{"$error":"#VALUE!"}},{"$f":"ADDRESS(ROW()+1+5,1)","v":"$A$302"},{"$f":"VALUE(RIGHT(LEFT(INDIRECT(M296),26),9))","v":864768},{"$f":"VALUE(RIGHT(INDIRECT(M296),3))","v":{"$error":"#VALUE!"}},{"$f":"ADDRESS(ROW()+2+5,1)","v":"$A$303"},{"$f":"VALUE(RIGHT(LEFT(INDIRECT(P296),26),9))","v":1308160},{"$f":"VALUE(RIGHT(INDIRECT(P296),3))","v":{"$error":"#VALUE!"}}]
["Write to file:     690688 bytes/sec",null,null,null,{"$f":"IF(LEN(E296)=5,ADDRESS(RIGHT(E296,2)+5,1),ADDRESS(RIGHT(E296,3)+5,1))","v":"$A$305"},"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",{"$f":"VALUE(MID(F297,16,5))","v":32768},{"$f":"MID(F297,28,9)","v":"MEMF_FAST"},{"$f":"MID(F297,39,4)","v":"LONG"},{"$f":"IF(LEN(J296)=5,ADDRESS(RIGHT(J296,2)+5,1),ADDRESS(RIGHT(J296,3)+5,1))","v":"$A$306"},{"$f":"VALUE(RIGHT(LEFT(INDIRECT(J297),26),9))","v":1679257},{"$f":"VALUE(RIGHT(INDIRECT(J297),3))","v":{"$error":"#VALUE!"}},{"$f":"IF(LEN(M296)=5,ADDRESS(RIGHT(M296,2)+5,1),ADDRESS(RIGHT(M296,3)+5,1))","v":"$A$307"},{"$f":"VALUE(RIGHT(LEFT(INDIRECT(M297),26),9))","v":1531904},{"$f":"VALUE(RIGHT(INDIRECT(M297),3))","v":{"$error":"#VALUE!"}},{"$f":"IF(LEN(P296)=5,ADDRESS(RIGHT(P296,2)+5,1),ADDRESS(RIGHT(P296,3)+5,1))","v":"$A$308"},{"$f":"VALUE(RIGHT(LEFT(INDIRECT(P297),26),9))","v":1957888},{"$f":"VALUE(RIGHT(INDIRECT(P297),3))","v":{"$error":"#VALUE!"}}]
["Read from file:    348436 bytes/sec",null,null,null,{"$f":"IF(LEN(E297)=5,ADDRESS(RIGHT(E297,2)+5,1),ADDRESS(RIGHT(E297,3)+5,1))","v":"$A$310"},"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",{"$f":"VALUE(MID(F298,16,6))","v":262144},{"$f":"MID(F298,29,9)","v":"MEMF_FAST"},{"$f":"MID(F298,40,4)","v":"LONG"},{"$f":"IF(LEN(J297)=5,ADDRESS(RIGHT(J297,2)+5,1),ADDRESS(RIGHT(J297,3)+5,1))","v":"$A$311"},1828152,{"$error":"#VALUE!"},{"$f":"IF(LEN(M297)=5,ADDRESS(RIGHT(M297,2)+5,1),ADDRESS(RIGHT(M297,3)+5,1))","v":"$A$312"},1632278,{"$error":"#VALUE!"},{"$f":"IF(LEN(P297)=5,ADDRESS(RIGHT(P297,2)+5,1),ADDRESS(RIGHT(P297,3)+5,1))","v":"$A$313"},2111444,{"$error":"#VALUE!"}]
[null,null,null,null,"$A$315","Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",{"$f":"VALUE(MID(F299,16,3))","v":512},{"$f":"MID(F299,26,9)","v":"MEMF_FAST"},{"$f":"MID(F299,37,4)","v":"WORD"},"$A$316",643904,{"$error":"#VALUE!"},"$A$317",660928,{"$error":"#VALUE!"},"$A$318",336448,{"$error":"#VALUE!"}]
["Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",null,null,null,"$A$320","Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",{"$f":"VALUE(MID(F300,16,4))","v":4096},{"$f":"MID(F300,27,9)","v":"MEMF_FAST"},{"$f":"MID(F300,38,4)","v":"WORD"},"$A$321",891904,{"$error":"#VALUE!"},"$A$322",879104,{"$error":"#VALUE!"},"$A$323",1174016,{"$error":"#VALUE!"}]
["Create file:       911360 bytes/sec",null,null,null,"$A$325","Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",{"$f":"VALUE(MID(F301,16,5))","v":32768},{"$f":"MID(F301,28,9)","v":"MEMF_FAST"},{"$f":"MID(F301,39,4)","v":"WORD"},"$A$326",1468628,{"$error":"#VALUE!"},"$A$327",1350710,{"$error":"#VALUE!"},"$A$328",1685445,{"$error":"#VALUE!"}]
["Write to file:     864768 bytes/sec",null,null,null,"$A$330","Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",{"$f":"VALUE(MID(F302,16,6))","v":262144},{"$f":"MID(F302,29,9)","v":"MEMF_FAST"},{"$f":"MID(F302,40,4)","v":"WORD"},"$A$331",1413521,{"$error":"#VALUE!"},"$A$332",1384790,{"$error":"#VALUE!"},"$A$333",1810118,{"$error":"#VALUE!"}]
["Read from file:   1308160 bytes/sec",null,null,null,"$A$335","Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",{"$f":"VALUE(MID(F303,16,3))","v":512},{"$f":"MID(F303,26,9)","v":"MEMF_FAST"},{"$f":"MID(F303,37,4)","v":"BYTE"},"$A$336",603533,{"$error":"#VALUE!"},"$A$337",526784,{"$error":"#VALUE!"},"$A$338",338901,{"$error":"#VALUE!"}]
[null,null,null,null,"$A$340","Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",{"$f":"VALUE(MID(F304,16,4))","v":4096},{"$f":"MID(F304,27,9)","v":"MEMF_FAST"},{"$f":"MID(F304,38,4)","v":"BYTE"},"$A$341",897536,{"$error":"#VALUE!"},"$A$342",651545,{"$error":"#VALUE!"},"$A$343",1175040,{"$error":"#VALUE!"}]
["Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",null,null,null,"$A$345","Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",{"$f":"VALUE(MID(F305,16,5))","v":32768},{"$f":"MID(F305,28,9)","v":"MEMF_FAST"},{"$f":"MID(F305,39,4)","v":"BYTE"},"$A$346",1442282,{"$error":"#VALUE!"},"$A$347",1264083,{"$error":"#VALUE!"},"$A$348",1687552,{"$error":"#VALUE!"}]
["Create file:      1679257 bytes/sec",null,null,null,"$A$350","Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",{"$f":"VALUE(MID(F306,16,6))","v":262144},{"$f":"MID(F306,29,9)","v":"MEMF_FAST"},{"$f":"MID(F306,40,4)","v":"BYTE"},"$A$351",1576080,{"$error":"#VALUE!"},"$A$352",1503569,{"$error":"#VALUE!"},"$A$353",1810118,{"$error":"#VALUE!"}]
["Write to file:    1531904 bytes/sec",null,null,null,"$A$355","Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",{"$f":"VALUE(MID(F307,16,3))","v":512},{"$f":"MID(F307,26,9)","v":"MEMF_CHIP"},{"$f":"MID(F307,37,4)","v":"LONG"},"$A$356",561024,{"$error":"#VALUE!"},"$A$357",507264,{"$error":"#VALUE!"},"$A$358",327959,{"$error":"#VALUE!"}]
["Read from file:   1957888 bytes/sec",null,null,null,"$A$360","Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",{"$f":"VALUE(MID(F308,16,4))","v":4096},{"$f":"MID(F308,27,9)","v":"MEMF_CHIP"},{"$f":"MID(F308,38,4)","v":"LONG"},"$A$361",762368,{"$error":"#VALUE!"},"$A$362",592896,{"$error":"#VALUE!"},"$A$363",829440,{"$error":"#VALUE!"}]
[null,null,null,null,"$A$365","Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",{"$f":"VALUE(MID(F309,16,5))","v":32768},{"$f":"MID(F309,28,9)","v":"MEMF_CHIP"},{"$f":"MID(F309,39,4)","v":"LONG"},"$A$366",905914,{"$error":"#VALUE!"},"$A$367",715012,{"$error":"#VALUE!"},"$A$368",1090904,{"$error":"#VALUE!"}]
["Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",null,null,null,"$A$370","Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",{"$f":"VALUE(MID(F310,16,6))","v":262144},{"$f":"MID(F310,29,9)","v":"MEMF_CHIP"},{"$f":"MID(F310,40,4)","v":"LONG"},"$A$371",1031809,{"$error":"#VALUE!"},"$A$372",735281,{"$error":"#VALUE!"},"$A$373",1135524,{"$error":"#VALUE!"}]
["Create file:      1828152 bytes/sec",null,null,null,"$A$375","Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",{"$f":"VALUE(MID(F311,16,3))","v":512},{"$f":"MID(F311,26,9)","v":"MEMF_CHIP"},{"$f":"MID(F311,37,4)","v":"WORD"},"$A$376",497920,{"$error":"#VALUE!"},"$A$377",417960,{"$error":"#VALUE!"},"$A$378",299072,{"$error":"#VALUE!"}]
["Write to file:    1632278 bytes/sec",null,null,null,"$A$380","Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",{"$f":"VALUE(MID(F312,16,4))","v":4096},{"$f":"MID(F312,27,9)","v":"MEMF_CHIP"},{"$f":"MID(F312,38,4)","v":"WORD"},"$A$381",670720,{"$error":"#VALUE!"},"$A$382",610816,{"$error":"#VALUE!"},"$A$383",828416,{"$error":"#VALUE!"}]
["Read from file:   2111444 bytes/sec",null,null,null,"$A$385","Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",{"$f":"VALUE(MID(F313,16,5))","v":32768},{"$f":"MID(F313,28,9)","v":"MEMF_CHIP"},{"$f":"MID(F313,39,4)","v":"WORD"},"$A$386",897753,{"$error":"#VALUE!"},"$A$387",835584,{"$error":"#VALUE!"},"$A$388",1041875,{"$error":"#VALUE!"}]
[null,null,null,null,"$A$390","Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",{"$f":"VALUE(MID(F314,16,6))","v":262144},{"$f":"MID(F314,29,9)","v":"MEMF_CHIP"},{"$f":"MID(F314,40,4)","v":"WORD"},"$A$391",916358,{"$error":"#VALUE!"},"$A$392",873813,{"$error":"#VALUE!"},"$A$393",1090929,{"$error":"#VALUE!"}]
["Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",null,null,null,{"$f":"IF(LEN(E314)=5,ADDRESS(RIGHT(E314,2)+5,1),ADDRESS(RIGHT(E314,3)+5,1))","v":"$A$395"},"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",{"$f":"VALUE(MID(F315,16,3))","v":512},{"$f":"MID(F315,26,9)","v":"MEMF_CHIP"},{"$f":"MID(F315,37,4)","v":"BYTE"},"$A$396",435456,{"$error":"#VALUE!"},"$A$397",465920,{"$error":"#VALUE!"},"$A$398",279197,{"$error":"#VALUE!"}]
["Create file:       643904 bytes/sec",null,null,null,"$A$400","Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",{"$f":"VALUE(MID(F316,16,4))","v":4096},{"$f":"MID(F316,27,9)","v":"MEMF_CHIP"},{"$f":"MID(F316,38,4)","v":"BYTE"},"$A$401",576000,{"$error":"#VALUE!"},"$A$402",537088,{"$error":"#VALUE!"},"$A$403",704000,{"$error":"#VALUE!"}]
["Write to file:     660928 bytes/sec",null,null,null,"$A$405","Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",{"$f":"VALUE(MID(F317,16,5))","v":32768},{"$f":"MID(F317,28,9)","v":"MEMF_CHIP"},{"$f":"MID(F317,39,4)","v":"BYTE"},"$A$406",744541,{"$error":"#VALUE!"},"$A$407",568633,{"$error":"#VALUE!"},"$A$408",852865,{"$error":"#VALUE!"}]
["Read from file:    336448 bytes/sec",null,null,null,"$A$410","Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",{"$f":"VALUE(MID(F318,16,6))","v":262144},{"$f":"MID(F318,29,9)","v":"MEMF_CHIP"},{"$f":"MID(F318,40,4)","v":"BYTE"},"$A$411",778645,{"$error":"#VALUE!"},"$A$412",601538,{"$error":"#VALUE!"},"$A$413",884341,{"$error":"#VALUE!"}]
[]
["Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer."]
["Create file:       891904 bytes/sec"]
["Write to file:     879104 bytes/sec"]
["Read from file:   1174016 bytes/sec"]
[]
["Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer."]
["Create file:      1468628 bytes/sec"]
["Write to file:    1350710 bytes/sec"]
["Read from file:   1685445 bytes/sec"]
[]
["Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer."]
["Create file:      1413521 bytes/sec"]
["Write to file:    1384790 bytes/sec"]
["Read from file:   1810118 bytes/sec"]
[]
["Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer."]
["Create file:       603533 bytes/sec"]
["Write to file:     526784 bytes/sec"]
["Read from file:    338901 bytes/sec"]
[]
["Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer."]
["Create file:       897536 bytes/sec"]
["Write to file:     651545 bytes/sec"]
["Read from file:   1175040 bytes/sec"]
[]
["Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer."]
["Create file:      1442282 bytes/sec"]
["Write to file:    1264083 bytes/sec"]
["Read from file:   1687552 bytes/sec"]
[]
["Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer."]
["Create file:      1576080 bytes/sec"]
["Write to file:    1503569 bytes/sec"]
["Read from file:   1810118 bytes/sec"]
[]
["Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.","CHIP RAM"]
["Create file:       561024 bytes/sec"]
["Write to file:     507264 bytes/sec"]
["Read from file:    327959 bytes/sec"]
[]
["Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer."]
["Create file:       762368 bytes/sec"]
["Write to file:     592896 bytes/sec"]
["Read from file:    829440 bytes/sec"]
[]
["Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer."]
["Create file:       905914 bytes/sec"]
["Write to file:     715012 bytes/sec"]
["Read from file:   1090904 bytes/sec"]
[]
["Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer."]
["Create file:      1031809 bytes/sec"]
["Write to file:     735281 bytes/sec"]
["Read from file:   1135524 bytes/sec"]
[]
["Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer."]
["Create file:       497920 bytes/sec"]
["Write to file:     417960 bytes/sec"]
["Read from file:    299072 bytes/sec"]
[]
["Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer."]
["Create file:       670720 bytes/sec"]
["Write to file:     610816 bytes/sec"]
["Read from file:    828416 bytes/sec"]
[]
["Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer."]
["Create file:       897753 bytes/sec"]
["Write to file:     835584 bytes/sec"]
["Read from file:   1041875 bytes/sec"]
[]
["Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer."]
["Create file:       916358 bytes/sec"]
["Write to file:     873813 bytes/sec"]
["Read from file:   1090929 bytes/sec"]
[]
["Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer."]
["Create file:       435456 bytes/sec"]
["Write to file:     465920 bytes/sec"]
["Read from file:    279197 bytes/sec"]
[]
["Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer."]
["Create file:       576000 bytes/sec"]
["Write to file:     537088 bytes/sec"]
["Read from file:    704000 bytes/sec"]
[]
["Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer."]
["Create file:       744541 bytes/sec"]
["Write to file:     568633 bytes/sec"]
["Read from file:    852865 bytes/sec"]
[]
["Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer."]
["Create file:       778645 bytes/sec"]
["Write to file:     601538 bytes/sec"]
["Read from file:    884341 bytes/sec"]
[]
["Average CPU Available: 9%  |  CPU Availability index: 444"]
[]
["Skipping 262144 byte MEMF_FAST test due to lack of memory."]
[]
["Skipping 512 byte MEMF_FAST test due to lack of memory."]
[]
["Skipping 4096 byte MEMF_FAST test due to lack of memory."]
[]
["Skipping 32768 byte MEMF_FAST test due to lack of memory."]
[]
["Skipping 262144 byte MEMF_FAST test due to lack of memory."]
[]
["Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer."]
["Create file:       131072 bytes/sec  |  CPU Available: 24%"]
["Write to file:     155948 bytes/sec  |  CPU Available: 29%"]
["Read from file:     85141 bytes/sec  |  CPU Available: 37%"]
[]
["Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer."]
["Create file:       215956 bytes/sec  |  CPU Available: 45%"]
["Write to file:     217138 bytes/sec  |  CPU Available: 52%"]
["Read from file:    436408 bytes/sec  |  CPU Available: 37%"]
[]
["Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer."]
["Create file:       612867 bytes/sec  |  CPU Available: 26%"]
["Write to file:     661897 bytes/sec  |  CPU Available: 35%"]
["Read from file:    692855 bytes/sec  |  CPU Available: 46%"]
[]
["Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer."]
["Create file:       719996 bytes/sec  |  CPU Available: 21%"]
["Write to file:     885407 bytes/sec  |  CPU Available: 23%"]
["Read from file:   1066677 bytes/sec  |  CPU Available: 27%"]
[]
["Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer."]
["Create file:       133167 bytes/sec  |  CPU Available: 13%"]
["Write to file:     156524 bytes/sec  |  CPU Available: 16%"]
["Read from file:     88868 bytes/sec  |  CPU Available: 27%"]
[]
["Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer."]
["Create file:       215202 bytes/sec  |  CPU Available: 42%"]
["Write to file:     217545 bytes/sec  |  CPU Available: 49%"]
["Read from file:    373108 bytes/sec  |  CPU Available: 27%"]
[]
["Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer."]
["Create file:       466535 bytes/sec  |  CPU Available: 20%"]
["Write to file:     492231 bytes/sec  |  CPU Available: 27%"]
["Read from file:    538652 bytes/sec  |  CPU Available: 32%"]
[]
["Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer."]
["Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer."]
["Create file:       131072 bytes/sec  |  CPU Available: 24%"]
["Write to file:     155948 bytes/sec  |  CPU Available: 29%"]
["Read from file:     85141 bytes/sec  |  CPU Available: 37%"]
[]
["Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer."]
["Create file:       215956 bytes/sec  |  CPU Available: 45%"]
["Write to file:     217138 bytes/sec  |  CPU Available: 52%"]
["Read from file:    436408 bytes/sec  |  CPU Available: 37%"]
[]
["Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer."]
["Create file:       612867 bytes/sec  |  CPU Available: 26%"]
["Write to file:     661897 bytes/sec  |  CPU Available: 35%"]
["Read from file:    692855 bytes/sec  |  CPU Available: 46%"]
[]
["Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer."]
["Create file:       719996 bytes/sec  |  CPU Available: 21%"]
["Write to file:     885407 bytes/sec  |  CPU Available: 23%"]
["Read from file:   1066677 bytes/sec  |  CPU Available: 27%"]
[]
["Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer."]
["Create file:       133167 bytes/sec  |  CPU Available: 13%"]
["Write to file:     156524 bytes/sec  |  CPU Available: 16%"]
["Read from file:     88868 bytes/sec  |  CPU Available: 27%"]
[]
["Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer."]
["Create file:       215202 bytes/sec  |  CPU Available: 42%"]
["Write to file:     217545 bytes/sec  |  CPU Available: 49%"]
["Read from file:    373108 bytes/sec  |  CPU Available: 27%"]
[]
["Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer."]
["Create file:       466535 bytes/sec  |  CPU Available: 20%"]
["Write to file:     492231 bytes/sec  |  CPU Available: 27%"]
["Read from file:    538652 bytes/sec  |  CPU Available: 32%"]
[]
["Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer."]
["Create file:       534987 bytes/sec  |  CPU Available: 15%"]
["Write to file:     613391 bytes/sec  |  CPU Available: 16%"]
["Read from file:    696517 bytes/sec  |  CPU Available: 19%"]
[]
["Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer."]
["Create file:       133204 bytes/sec  |  CPU Available: 13%"]
["Write to file:     155820 bytes/sec  |  CPU Available: 16%"]
["Read from file:     90052 bytes/sec  |  CPU Available: 26%"]
[]
["Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer."]
["Create file:       216548 bytes/sec  |  CPU Available: 42%"]
["Write to file:     217622 bytes/sec  |  CPU Available: 49%"]
["Read from file:    390656 bytes/sec  |  CPU Available: 24%"]
[]
["Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer."]
["Create file:       468871 bytes/sec  |  CPU Available: 19%"]
["Write to file:     496361 bytes/sec  |  CPU Available: 26%"]
["Read from file:    565807 bytes/sec  |  CPU Available: 29%"]
[]
["Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer."]
["Create file:       541488 bytes/sec  |  CPU Available: 14%"]
["Write to file:     617957 bytes/sec  |  CPU Available: 15%"]
["Read from file:    708497 bytes/sec  |  CPU Available: 18%"]
[]
["Average CPU Available: 25%  |  CPU Availability index: 108"]

{"sheet":"KT_BT","index":3,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[]}
[]
["Aligned buffer","(Více položek)"]
[]
[null,"Popisky sloupců"]
[null,"Samsung 356 MB",null,null,"Sandisk CF 4GB"]
["Popisky řádků","Průměr z Create file in bytes/sec","Průměr z Write to file in bytes/sec","Průměr z Read from file in bytes/sec","Průměr z Create file in bytes/sec","Průměr z Write to file in bytes/sec","Průměr z Read from file in bytes/sec"]
["MEMF_CHIP",431334.63888888888,463810.29166666669,537061.71527777775,664446.6631944445,643792.04861111112,800465.48958333337]
[512,264705.84722222225,297130.31944444444,206699.06944444444,358899.66666666669,376152.95833333331,233600.13888888888]
["Amiga 1200 (no FAST]",132164.22222222222,155022.44444444444,86794,156192.77777777778,185917.44444444444,122003.55555555556]
["MemoryMaster1200(9MB)",210648.77777777778,240054.33333333334,180353,268664.11111111112,289448,198293.88888888888]
["Blizzard 1200 (4MB)",214255.11111111112,252363.66666666666,183322.66666666666,267542.55555555556,303864.88888888888,198510.55555555556]
["Blizzard 1220 (4+4MB)",265409.88888888888,294119.77777777775,218874.44444444444,351668.22222222225,390099.11111111112,244346.88888888888]
["Blizzard 1230 IV (64MB)",312948.88888888888,375215.55555555556,249564.88888888888,440921,455325.77777777775,277719.44444444444]
["Blizzard 1240 (64MB)",315548.16666666669,346042.27777777775,233895.61111111112,439322.61111111112,451463.83333333331,263187.72222222225]
["Blizzard 1260 (128MB)",351123.55555555556,368182.22222222225,266892.33333333331,507563.44444444444,481640.77777777775,301551.33333333331]
[4096,210657.80555555556,216507.77777777778,556956.79166666663,578572.27777777775,550945.6944444445,746345.65277777775]
["Amiga 1200 (no FAST]",215704.22222222222,217453.44444444444,400208.33333333331,356955.22222222225,368418.44444444444,555571.77777777775]
["MemoryMaster1200(9MB)",191419.55555555556,213589.44444444444,553597.33333333337,530090.66666666663,506698.44444444444,771640.88888888888]
["Blizzard 1200 (4MB)",195518.88888888888,216544.55555555556,578447.5555555555,534097.22222222225,529164.88888888888,769763.5555555555]
["Blizzard 1220 (4+4MB)",215680,216369.55555555556,583039.77777777775,607548.66666666663,587358.4444444445,790016]
["Blizzard 1230 IV (64MB)",217624.55555555556,217885,635297,695553,622203.88888888888,840527.77777777775]
["Blizzard 1240 (64MB)",217507.55555555556,217321.05555555556,568318.61111111112,618410.83333333337,588297.88888888888,728077.61111111112]
["Blizzard 1260 (128MB)",214300.11111111112,215578.11111111112,568427.11111111112,667511.77777777775,617125.66666666663,787090]
[32768,570918.66666666663,613726.52777777775,597839.65277777775,862620.97222222225,807109.9305555555,1076353.6666666667]
["Amiga 1200 (no FAST]",505848.88888888888,546038.88888888888,587277.33333333337,642010,716989.4444444445,939842]
["MemoryMaster1200(9MB)",549694.88888888888,621967.5555555555,588108.4444444445,851142,871408,1195963.5555555555]
["Blizzard 1200 (4MB)",553214.22222222225,633436.66666666663,594195.5555555555,854615.77777777775,872793.4444444445,1188933.111111111]
["Blizzard 1220 (4+4MB)",603430,626689.33333333337,598507,934779,825810.5555555555,1156891.6666666667]
["Blizzard 1230 IV (64MB)",598791,643851.66666666663,597870.22222222225,1033841.5555555555,975077.5555555555,1188048.4444444445]
["Blizzard 1240 (64MB)",556756.66666666663,591336.27777777775,581626.88888888888,862478.9444444445,715567.61111111112,972820]
["Blizzard 1260 (128MB)",642857,655155.5555555555,653504.88888888888,859621.5555555555,763665.22222222225,995510.5555555555]
[262144,679056.23611111112,727876.54166666663,786751.34722222225,857693.73611111112,840959.61111111112,1145562.5]
["Amiga 1200 (no FAST]",601237,701628.66666666663,831606.11111111112,698743.5555555555,715019.66666666663,1032452.5555555555]
["MemoryMaster1200(9MB)",686623.11111111112,760673.22222222225,785289.88888888888,761498.77777777775,911469.11111111112,1292092.2222222222]
["Blizzard 1200 (4MB)",685343.88888888888,740780.11111111112,757207.11111111112,813442.77777777775,901061.77777777775,1283015.111111111]
["Blizzard 1220 (4+4MB)",643217.66666666663,710158.77777777775,803718.77777777775,896558.11111111112,914635.11111111112,1230324.2222222222]
["Blizzard 1230 IV (64MB)",730069.4444444445,769339.22222222225,794570.77777777775,1019916.1111111111,962610.66666666663,1249798]
["Blizzard 1240 (64MB)",635371.61111111112,653535.27777777775,729491.61111111112,872102.5555555555,750097.83333333337,1019824.8333333334]
["Blizzard 1260 (128MB)",815215.5555555555,833361.77777777775,862634.88888888888,927185.4444444445,822684.88888888888,1037168.2222222222]
["MEMF_FAST",558202.01984126982,581352.47619047621,714540.90476190473,972463.31746031751,926379.21428571432,1199422.5198412698]
[512,321634.71428571426,336576.6984126984,239958.79365079364,448980.50793650793,471500.52380952379,270075.22222222225]
["MemoryMaster1200(9MB)",220018.33333333334,270257.33333333331,184011.11111111112,277586.77777777775,310471.77777777775,202723.66666666666]
["Blizzard 1200 (4MB)",222493.88888888888,264838,182003.66666666666,277985.55555555556,324411.33333333331,203181.44444444444]
["Blizzard 1220 (4+4MB)",276958.55555555556,310767.33333333331,234275.77777777778,379204.33333333331,417025.55555555556,258356.88888888888]
["Blizzard 1230 IV (64MB)",375053,375823.66666666669,263060.55555555556,495837.66666666669,513957.44444444444,299375.88888888888]
["Blizzard 1240 (64MB)",384815.38888888888,375749.11111111112,257547.77777777778,536417.0555555555,560212.4444444445,292831.27777777775]
["Blizzard 1260 (128MB)",387288.44444444444,382852.33333333331,301264.88888888888,639415.11111111112,614212.66666666663,341226.11111111112]
[4096,215695.49206349207,216393.03174603175,723800.4444444445,734206.98412698414,687397.39682539681,1033467.9365079365]
["MemoryMaster1200(9MB)",213406.88888888888,216368.11111111112,643845.88888888888,571289.5555555555,580395.88888888888,897592.88888888888]
["Blizzard 1200 (4MB)",211041.77777777778,213244.88888888888,627209.66666666663,574988.5555555555,553583.11111111112,896341.33333333337]
["Blizzard 1220 (4+4MB)",217277.44444444444,217023.11111111112,728980.77777777775,622959.22222222225,663597.88888888888,1028551.1111111111]
["Blizzard 1230 IV (64MB)",217080,217231.11111111112,771659.5555555555,841329.77777777775,780463,1137436.4444444445]
["Blizzard 1240 (64MB)",216759.33333333334,216719.44444444444,746980.16666666663,813710.22222222225,718178,1027384.8888888889]
["Blizzard 1260 (128MB)",217543.66666666666,217445.11111111112,800946.88888888888,901461.33333333337,797385.88888888888,1219584]
[32768,776572.60317460319,798972.65079365077,814952.8412698413,1306079.2857142857,1219297.746031746,1672083.3015873015]
["MemoryMaster1200(9MB)",651195.66666666663,689929.11111111112,732026.77777777775,933463.33333333337,959997.4444444445,1542703.4444444445]
["Blizzard 1200 (4MB)",652928.77777777775,685308.66666666663,723019.22222222225,965705.11111111112,1079163.2222222222,1530525.7777777778]
["Blizzard 1220 (4+4MB)",751418.4444444445,807286,879794.4444444445,1234131.111111111,1058341.888888889,1775795.6666666667]
["Blizzard 1230 IV (64MB)",832372.4444444445,854375.22222222225,839809.4444444445,1543017.888888889,1348565.6666666667,1904779.888888889]
["Blizzard 1240 (64MB)",801327.11111111112,806844.38888888888,791726.33333333337,1465390.888888889,1378282.3333333333,1587069.7777777778]
["Blizzard 1260 (128MB)",945438.66666666663,942220.77777777775,946567.33333333337,1535455.7777777778,1332451.3333333333,1776638.7777777778]
[262144,918905.26984126982,973467.52380952379,1079451.5396825396,1400586.4920634921,1327321.1904761905,1822063.6190476189]
["MemoryMaster1200(9MB)",827329.66666666663,917868.88888888888,946732.4444444445,1147883.888888889,1190924.3333333333,1707080]
["Blizzard 1200 (4MB)",796460.66666666663,890717.88888888888,919168.5555555555,1087653.888888889,1133831,1692588.4444444445]
["Blizzard 1220 (4+4MB)",792185,838103.22222222225,1074000.888888889,1320633.6666666667,1383093.6666666667,1944450.888888889]
["Blizzard 1230 IV (64MB)",915343.77777777775,943667,1134562.6666666667,1581610.888888889,1366905.4444444445,2074715.3333333333]
["Blizzard 1240 (64MB)",918042.77777777775,953970.83333333337,1077891.7777777778,1533607.388888889,1371835.111111111,1712525.3333333333]
["Blizzard 1260 (128MB)",1264932.2222222222,1315974,1325912.6666666667,1599108.3333333333,1472823.6666666667,1910560]

{"sheet":"BytovéTesty","index":4,"n_rows":1153,"n_cols":14,"rows_kept":1153,"cut":false,"hidden":false,"merged":[]}
["File System","Disk","Accelerator","Test #","Type of test","Size (bytes)","Tested Memory","Aligned buffer","Create file in bytes/sec","CPU Available","Write to file in bytes/sec","CPU Available2","Read from file in bytes/sec","CPU Available3"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",133231,0.22,152153,0.31,83478,0.38]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",215498,0.45,216979,0.52,420352,0.39]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",589824,0.28999999999999998,641468,0.38,711814,0.45]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",720896,0.21,853786,0.26,1084293,0.26]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",132271,0.14000000000000001,156435,0.16,86175,0.28999999999999998]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",214852,0.42,217409,0.49,384495,0.25]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",451832,0.22,501301,0.26,550208,0.31]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",534987,0.15,619494,0.15,729058,0.16]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",132190,0.14000000000000001,154649,0.17,89710,0.26]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",216735,0.42,217464,0.49,376178,0.27]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",457493,0.22,480147,0.28999999999999998,525102,0.34]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",1,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",546803,0.13,618724,0.15,713758,0.17]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",130399,0.24,159576,0.27,84533,0.37]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",215686,0.45,219236,0.51,455395,0.35]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",590231,0.28999999999999998,660250,0.36,661897,0.49]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",755276,0.17,883631,0.23,1097647,0.25]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",130207,0.16,152025,0.18,87654,0.28000000000000003]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",214986,0.42,216143,0.49,380868,0.26]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",457722,0.22,489135,0.28000000000000003,503179,0.37]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",524905,0.16,610384,0.17,694839,0.2]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",133737,0.13,152072,0.18,85535,0.28999999999999998]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",215875,0.42,217545,0.49,384415,0.25]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",457265,0.21,491560,0.27,535982,0.33]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",2,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",531795,0.15,611884,0.16,693169,0.2]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",131072,0.24,155948,0.28999999999999998,85141,0.37]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",215956,0.45,217138,0.52,436408,0.37]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",612867,0.26,661897,0.35,692855,0.46]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",719996,0.21,885407,0.23,1066677,0.27]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",133167,0.13,156524,0.16,88868,0.27]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",215202,0.42,217545,0.49,373108,0.27]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",466535,0.2,492231,0.27,538652,0.32]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",534987,0.15,613391,0.16,696517,0.19]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",133204,0.13,155820,0.16,90052,0.26]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",216548,0.42,217622,0.49,390656,0.24]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",468871,0.19,496361,0.26,565807,0.28999999999999998]
["PFS3_18.5_020/030","Samsung 356 MB","Amiga 1200 (no FAST]",3,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",541488,0.14000000000000001,617957,0.15,708497,0.18]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",171008,0,209879,0.04,132574,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",370502,0.06,413385,0.09,671232,0.02]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",808985,0.01,943816,7.0000000000000007E-2,1255902,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",891862,0,1048576,0.06,1407264,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",152812,0.01,163054,0.12,122736,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",359531,0.04,391168,0.08,499137,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",573440,0,595781,0.11,781359,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",607406,0.02,553596,0.23,845625,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",152896,0.01,177107,0.05,121746,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",351596,0.06,332979,0.22,497601,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",561737,0.02,629996,0.06,781359,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",617191,0,647269,0.1,845625,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",166898,0.02,193396,0.12,128207,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",368921,0.06,357485,0.21,672768,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",809995,0.01,856946,0.15,1258421,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",855851,0.04,756184,0.32,1407264,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",148205,0.03,178253,0.04,113834,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",344872,7.0000000000000007E-2,334764,0.21,499649,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",560451,0.02,629996,0.06,781359,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",617957,0,652911,0.09,845625,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",150189,0.02,182098,0.02,121569,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",352327,0.05,368547,0.14000000000000001,500224,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",556974,0.03,644750,0.03,779413,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",611884,0.01,685557,0.05,843532,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Skipping byte MEMF_FAST test due to lack of memory.","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a","n/a"]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",168085,0.02,207334,0.06,127792,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",367898,0.06,404543,0.11,666303,0.02]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",782336,0.04,875170,0.13,1259993,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",858966,0.04,751667,0.32,1409024,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",146093,0.05,180370,0.03,114133,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",344958,7.0000000000000007E-2,334764,0.21,496329,0.02]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",562435,0.02,628427,0.06,781359,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",617191,0,651289,0.09,842489,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",149549,0.03,181766,0.02,115441,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",351992,0.06,378131,0.11,496903,0.02]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",561737,0.02,648023,0.03,779413,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",610384,0.01,688128,0.04,845625,0]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",220716,0.28000000000000003,266462,0.3,196302,0.12]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",217088,0.66,218269,0.7,771072,0.31]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",790670,0.39,859956,0.45,679783,0.66]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",955567,0.33,1073294,0.38,938540,0.57999999999999996]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",215955,0.23,271498,0.17,183634,0.1]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",215552,0.65,217866,0.69,642560,0.26]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",592438,0.4,612104,0.45,567924,0.57999999999999996]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",781547,0.27,839377,0.31,804122,0.45]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",217444,0.22,273216,0.17,182395,0.11]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",215875,0.65,220132,0.69,649728,0.26]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",589087,0.4,599116,0.46,552909,0.59]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",793414,0.26,882529,0.28000000000000003,818177,0.45]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",217088,0.27,267486,0.27,188385,0.14000000000000001]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",216494,0.64,216465,0.68,619008,0.32]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",607267,0.38,664326,0.41,637382,0.55000000000000004]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",731712,0.3,809086,0.33,803137,0.48]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",213925,0.19,236258,0.23,179369,0.09]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",134679,0.42,215040,0.65,548864,0.28000000000000003]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",554284,0.33,584267,0.37,566511,0.49]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",671344,0.24,729940,0.26,770068,0.35]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",214986,0.19,229539,0.25,184442,7.0000000000000007E-2]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",216035,0.61,217033,0.65,537600,0.3]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",577302,0.3,606208,0.34,513136,0.54]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",1,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",677124,0.24,758921,0.23,746201,0.37]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",233186,0.23,272320,0.28000000000000003,191144,0.14000000000000001]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",214825,0.66,216708,0.7,714752,0.36]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",792642,0.39,861027,0.45,823296,0.59]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",938540,0.34,1086938,0.37,1135524,0.49]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",216996,0.22,273024,0.17,180306,0.12]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",213317,0.66,215444,0.69,573440,0.34]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",598016,0.39,636588,0.43,739527,0.46]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",770068,0.28000000000000003,814306,0.33,858966,0.42]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",216100,0.23,274141,0.16,174826,0.15]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",214474,0.65,217572,0.69,617472,0.28999999999999998]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",597269,0.39,625125,0.44,768127,0.44]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",791497,0.26,814111,0.33,877061,0.41]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",215750,0.27,269342,0.26,189368,0.14000000000000001]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",210917,0.65,215148,0.68,631296,0.31]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",632508,0.35,753053,0.33,648830,0.54]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",728177,0.31,816139,0.32,804122,0.48]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",212288,0.2,229246,0.25,175124,0.12]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",112984,0.37,214206,0.65,519405,0.32]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",559055,0.32,582813,0.37,611343,0.45]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",648871,0.27,734386,0.26,818177,0.31]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",212069,0.2,232832,0.24,174420,0.12]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",210654,0.62,215148,0.65,515451,0.33]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",559752,0.32,589087,0.36,604696,0.46]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",2,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",671344,0.24,716418,0.27,838344,0.3]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",237474,0.22,269662,0.28999999999999998,188032,0.16]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",210522,0.67,215121,0.7,647086,0.42]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",756813,0.42,833500,0.46,879540,0.56999999999999995]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",884341,0.38,1054969,0.39,1234383,0.45]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",212773,0.24,267870,0.18,183547,0.1]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",212161,0.66,214260,0.69,622326,0.28999999999999998]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",573948,0.42,588768,0.47,779413,0.43]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",774809,0.27,861056,0.28999999999999998,952096,0.36]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",209521,0.25,264123,0.19,175914,0.14000000000000001]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",206848,0.67,211941,0.69,556177,0.36]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",569878,0.42,593178,0.47,797722,0.42]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",756184,0.28999999999999998,834240,0.31,901723,0.39]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",204761,0.31,253922,0.3,181925,0.17]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",202271,0.67,203854,0.7,519680,0.43]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",655360,0.33,696320,0.38,651289,0.54]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",736179,0.3,842489,0.3,816139,0.47]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",201478,0.24,220416,0.28000000000000003,169495,0.14000000000000001]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",201333,0.64,203854,0.67,502272,0.34]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",233093,0.22,535906,0.42,555666,0.5]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",630153,0.28999999999999998,701601,0.28999999999999998,767250,0.36]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",203494,0.23,221448,0.28000000000000003,180649,0.09]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",217409,0.61,221557,0.64,588800,0.23]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",568633,0.32,585728,0.36,504123,0.54]
["PFS3_18.5_020/030","Samsung 356 MB","MemoryMaster1200(9MB)",3,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",684704,0.23,737079,0.25,704171,0.41]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",295515,0.03,347028,0.08,214949,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",572928,0.13,632320,0.15,1043456,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1255902,0.02,1349992,0.12,1959534,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1400272,0.01,1350926,0.2,2200715,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",269584,0.03,315736,0.03,197184,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",560640,0.12,464035,0.35,823808,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",927473,0.05,937968,0.16,1337719,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1026757,0.03,1039480,0.14000000000000001,1459960,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",262720,0.06,314171,0.04,197312,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",560640,0.12,467851,0.34,823296,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",607748,0.04,719098,0.35,1337719,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1013274,0.05,1132720,0.06,1461769,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",287628,0.03,299866,0.18,209701,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",553472,0.12,574976,0.18,859648,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",938560,0.04,1039085,0.06,1393252,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",1025502,0.02,1105818,7.0000000000000007E-2,1511750,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",262454,0.01,293120,0.05,190696,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",522240,0.08,520704,0.17,726016,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",818177,0.01,637382,0.3,1097707,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",861056,0.02,911805,7.0000000000000007E-2,1181404,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",262431,0.01,263327,0.14000000000000001,193039,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",521216,0.09,449991,0.28000000000000003,732672,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",796728,0.04,763090,0.17,1099076,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",420776,0.03,911805,7.0000000000000007E-2,1179966,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",296158,0.03,343443,0.09,213413,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",584704,0.11,635110,0.15,1042432,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1242078,0.04,1190447,0.22,1957888,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1376256,0.03,1553445,0.08,2198001,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",271198,0.03,263440,0.19,197646,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",562496,0.12,613888,0.14000000000000001,822784,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",971205,0.01,713399,0.35,1336051,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1018034,0.04,1128541,0.06,1459960,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",268288,0.03,270686,0.17,195047,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",577536,0.1,585216,0.18,825344,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",606194,0.04,984674,0.11,1336051,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1051124,0.01,1097647,0.09,1459960,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",292032,0.01,303706,0.16,211749,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",551424,0.12,601600,0.14000000000000001,851968,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",917504,0.06,1030903,7.0000000000000007E-2,1389167,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",1002030,0.05,765383,0.35,1513607,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",256607,0.03,267453,0.13,191424,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",521216,0.09,425697,0.32,727040,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",808985,0.02,840623,0.08,1100448,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",855851,0.03,680472,0.3,1182844,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",257375,0.03,255009,0.17,191592,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",514048,0.1,443793,0.28999999999999998,732160,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",805904,0.02,838631,0.08,1097707,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",415644,0.04,898412,0.08,1181404,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",294791,0.03,356224,0.06,214309,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",583974,0.12,615424,0.17,1046016,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1242078,0.04,1313174,0.14000000000000001,1951352,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1371114,0.03,1543915,0.09,2203435,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",272413,0.02,271198,0.17,197671,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",570880,0.1,595319,0.17,828416,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",951988,0.03,718703,0.35,1336051,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1023000,0.03,764453,0.36,1459960,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",267614,0.04,312320,0.04,196982,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",567808,0.11,614400,0.14000000000000001,822784,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",596504,7.0000000000000007E-2,712522,0.36,1331966,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1051124,0.01,1107192,0.08,1459960,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",283740,0.04,340800,7.0000000000000007E-2,212453,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",566272,0.09,480407,0.31,858112,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",958464,0.02,1011712,0.09,1390901,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",1024250,0.02,1127154,0.05,1513607,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",258207,0.02,286108,7.0000000000000007E-2,192847,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",517120,0.09,531303,0.15,726528,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",807978,0.02,836542,0.09,1097707,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",855851,0.03,897314,0.08,1181404,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",257503,0.03,295643,0.04,191144,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",503808,0.12,531815,0.15,730624,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",807978,0.02,844704,0.08,1097707,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",392529,0.06,905059,7.0000000000000007E-2,1182844,0]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",242816,0.21,272925,0.28000000000000003,194319,0.13]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",216494,0.66,221128,0.69,790528,0.28999999999999998]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",824300,0.37,853929,0.45,783493,0.61]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",916358,0.36,1053684,0.39,1038194,0.53]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",219684,0.22,272669,0.17,183657,0.1]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",217057,0.65,217622,0.69,603648,0.31]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",616953,0.38,641468,0.43,626688,0.54]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",746201,0.3,849843,0.3,867388,0.41]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",218916,0.22,272883,0.17,181289,0.12]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",216708,0.65,217088,0.69,600610,0.31]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",612104,0.38,634087,0.44,664326,0.51]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",772906,0.28000000000000003,807093,0.34,775765,0.48]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",218726,0.27,273984,0.25,192576,0.12]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",213397,0.65,218514,0.68,673280,0.26]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",610304,0.38,697799,0.38,715012,0.5]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",767250,0.27,826150,0.31,807093,0.47]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",213898,0.2,241185,0.22,179584,0.09]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",135710,0.42,214959,0.65,539997,0.28999999999999998]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",580181,0.3,616953,0.33,567216,0.49]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",662457,0.25,710242,0.28000000000000003,719098,0.39]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",212742,0.2,240545,0.22,176384,0.11]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",213264,0.62,218514,0.64,560451,0.27]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",588353,0.28999999999999998,602112,0.35,565807,0.49]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",1,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",643298,0.27,711118,0.28000000000000003,722073,0.39]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",242984,0.21,273629,0.28000000000000003,188304,0.16]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",214717,0.67,218133,0.7,710415,0.36]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",807978,0.38,879240,0.44,774144,0.61]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",924838,0.35,1067994,0.38,1053684,0.53]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",214104,0.24,265091,0.2,183337,0.11]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",212188,0.66,215013,0.69,646656,0.26]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",590231,0.4,612867,0.46,692855,0.49]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",748982,0.3,830175,0.32,861056,0.42]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",215653,0.23,264233,0.2,179859,0.12]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",210680,0.66,215471,0.69,653312,0.25]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",599862,0.39,615418,0.45,674154,0.51]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",734386,0.31,807093,0.34,856887,0.42]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",215589,0.28000000000000003,275136,0.25,188736,0.14000000000000001]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",212267,0.65,214744,0.68,651776,0.28000000000000003]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",638976,0.35,798720,0.28999999999999998,705647,0.5]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",785803,0.26,831188,0.31,785803,0.49]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",210432,0.21,243105,0.21,172564,0.13]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",124792,0.4,215121,0.65,534016,0.3]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",562435,0.32,598372,0.35,560451,0.5]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",637819,0.28000000000000003,726423,0.26,760756,0.36]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",210368,0.21,245831,0.2,174420,0.12]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",210759,0.62,212912,0.65,527724,0.31]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",532480,0.36,573948,0.38,597269,0.46]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",2,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",652911,0.26,692337,0.3,802154,0.33]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",239930,0.22,260084,0.32,189200,0.15]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",206383,0.68,208703,0.71,621039,0.44]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",748982,0.43,812058,0.48,835584,0.57999999999999996]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",866326,0.39,957895,0.44,1093606,0.51]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",204774,0.27,253153,0.23,168682,0.18]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",200964,0.68,200428,0.71,498763,0.43]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",535237,0.46,561737,0.5,735441,0.46]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",732601,0.31,800195,0.35,888623,0.4]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",203584,0.27,248875,0.24,169386,0.17]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",204185,0.67,205618,0.7,519916,0.4]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",540712,0.45,556974,0.5,720488,0.47]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",725548,0.32,842489,0.31,837314,0.43]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",216676,0.27,275037,0.25,200077,0.09]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",216654,0.65,217948,0.68,623104,0.32]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",623570,0.36,661072,0.41,587620,0.59]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",724676,0.31,793414,0.34,761677,0.5]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",214249,0.2,239522,0.22,183314,7.0000000000000007E-2]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",216251,0.61,218807,0.64,561664,0.27]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",269393,0.19,570587,0.38,542732,0.51]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",653725,0.26,695677,0.3,739792,0.38]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",215616,0.19,236928,0.24,182249,0.08]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",216576,0.61,217382,0.65,534016,0.3]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",573236,0.31,581367,0.37,506006,0.54]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1200 (4MB)",3,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",640156,0.28000000000000003,680472,0.31,716418,0.4]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",301978,0.01,352991,7.0000000000000007E-2,216548,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",584704,0.12,495554,0.33,1035264,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1193049,7.0000000000000007E-2,1366356,0.1,1930898,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1340137,0.05,1519206,0.1,2168351,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",268702,0.04,310089,0.05,195599,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",578048,0.1,601088,0.16,825856,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",930399,0.05,1022721,0.08,1333628,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1013274,0.04,1123015,7.0000000000000007E-2,1454559,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",257183,0.08,313560,0.04,196647,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",553984,0.13,605184,0.15,824832,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",939730,0.04,1005103,0.1,1329538,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",489135,0.05,1090929,0.09,1454559,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",284721,0.04,345828,0.05,210725,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",568121,0.09,586240,0.16,857088,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",907044,7.0000000000000007E-2,1022981,7.0000000000000007E-2,1386810,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",1000796,0.04,765383,0.35,1501696,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",242755,0.08,295707,0.04,193423,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",507904,0.11,537088,0.15,729088,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",819200,0.01,635797,0.3,1090904,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",875976,0,888623,0.09,1173779,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",262614,0.01,262912,0.14000000000000001,192975,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",522099,0.08,439588,0.3,730112,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",819200,0.01,829414,0.09,1088175,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",858966,0.02,916358,0.06,1172320,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",294235,0.04,352384,7.0000000000000007E-2,216356,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",600064,0.09,601600,0.19,1042432,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1262507,0.02,1309083,0.14000000000000001,1929216,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1393348,0.01,947508,0.43,2171031,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",271070,0.03,316477,0.03,199374,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",566587,0.11,615167,0.14000000000000001,825344,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",954883,0.03,966656,0.13,1333628,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1029277,0.03,1108569,0.08,1454559,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",266846,0.04,304064,7.0000000000000007E-2,198670,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",573952,0.1,476724,0.33,829440,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",607676,0.03,994085,0.11,1331966,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1056257,0,743441,0.38,1452768,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",293787,0.01,346004,0.05,212581,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",561474,0.1,587264,0.16,854016,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",956073,0.02,992845,0.1,1386810,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",1021754,0.02,1101717,7.0000000000000007E-2,1503569,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",257855,0.03,286717,7.0000000000000007E-2,192271,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",513917,0.1,543232,0.14000000000000001,729088,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",791655,0.04,854995,7.0000000000000007E-2,1093632,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",838344,0.05,664055,0.31,1173779,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",254913,0.04,265600,0.13,190568,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",524144,0.08,529769,0.16,720896,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",795735,0.03,849843,7.0000000000000007E-2,1089546,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",385600,0.08,894035,0.08,1173779,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",300995,0.01,354304,0.06,213194,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",570678,0.14000000000000001,633344,0.15,1033216,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1255902,0.02,1341810,0.12,1929216,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1388200,0.01,1470882,0.12,2168351,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",273664,0.02,307097,0.06,197774,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",572928,0.1,472423,0.34,822272,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",931559,0.05,1014539,0.09,1327104,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1023000,0.03,1111333,0.08,1454559,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",267197,0.04,308736,0.06,194471,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",573952,0.1,481164,0.33,828416,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",615641,0.03,692116,0.37,1329538,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1056257,0,1089596,0.09,1454559,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",291529,0.02,343253,0.06,211493,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",566784,0.09,482695,0.31,857088,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",968331,0.01,1002267,0.09,1382719,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",1043359,0,1086938,0.08,1503569,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",257470,0.03,298240,0.03,190096,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",518144,0.09,519680,0.17,727552,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",815104,0.02,841671,0.08,1092266,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",878149,0,898412,0.08,1170866,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",262239,0.01,290523,0.06,192463,0.03]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",524288,0.08,536928,0.14000000000000001,722944,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",819200,0.01,825328,0.1,1089536,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",418041,0.05,894035,0.08,1173779,0]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",268696,0.37,374801,0.27,251488,0.15]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",219483,0.73,218323,0.75,851968,0.36]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",737280,0.5,797722,0.51,849843,0.61]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",898412,0.43,935076,0.47,1097647,0.54]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",276782,0.3,270720,0.39,228782,0.17]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",219693,0.72,217861,0.75,726016,0.34]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",662723,0.45,750848,0.43,877349,0.48]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",779610,0.39,838344,0.41,960234,0.46]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",279616,0.28999999999999998,274653,0.38,236036,0.14000000000000001]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",219593,0.72,218405,0.75,723968,0.34]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",670068,0.44,767171,0.42,902958,0.46]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",738886,0.42,829165,0.41,883631,0.51]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",282624,0.28999999999999998,352039,0.25,247329,0.12]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",217758,0.7,221101,0.72,601360,0.31]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",647218,0.39,652911,0.44,620266,0.48]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",779610,0.31,813101,0.34,807093,0.35]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",192079,0.19,278737,0.3,214885,0.15]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",220313,0.66,218460,0.69,600576,0.31]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",607267,0.34,602442,0.39,604696,0.49]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",630912,0.35,676292,0.34,723806,0.42]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",281600,0.2,279899,0.28999999999999998,212682,0.15]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",218542,0.66,219802,0.68,626146,0.27]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",605451,0.34,601360,0.39,578738,0.51]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",1,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",605928,0.37,643298,0.38,731712,0.41]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",276703,0.34,381301,0.23,242792,0.15]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",219373,0.73,218002,0.75,784896,0.4]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",817157,0.44,853929,0.48,842722,0.61]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",879240,0.44,905059,0.49,979367,0.59]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",284316,0.26,285111,0.35,228387,0.14000000000000001]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",218944,0.72,217518,0.74,781312,0.28000000000000003]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",760904,0.36,866186,0.34,875449,0.47]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",744359,0.42,788640,0.44,1044658,0.42]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",279517,0.27,277568,0.36,226147,0.14000000000000001]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",215498,0.72,218084,0.74,681132,0.37]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",786432,0.34,794624,0.4,886615,0.47]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",760756,0.4,793414,0.44,1139756,0.36]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",278941,0.28999999999999998,329728,0.28999999999999998,230406,0.16]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",217006,0.7,218112,0.72,570368,0.34]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",626688,0.41,689637,0.4,591701,0.5]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",563750,0.28999999999999998,803137,0.34,761677,0.39]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",273497,0.22,274823,0.3,212874,0.14000000000000001]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",217758,0.66,218460,0.69,558220,0.35]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",598372,0.35,616185,0.37,621252,0.47]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",649675,0.33,667275,0.35,868452,0.3]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",276317,0.21,269265,0.31,209931,0.15]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",216548,0.67,218002,0.69,582144,0.32]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",590231,0.35,616185,0.37,604696,0.49]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",2,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",647269,0.33,667275,0.35,899513,0.28000000000000003]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",276125,0.34,374077,0.24,236292,0.16]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",215068,0.73,215364,0.75,715264,0.45]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",807978,0.44,877349,0.46,918156,0.57999999999999996]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",834240,0.47,879240,0.5,1318761,0.45]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",275377,0.28000000000000003,283126,0.35,230016,0.12]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",214987,0.72,215094,0.74,625366,0.42]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",767171,0.36,802816,0.39,866186,0.48]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",755276,0.41,780577,0.44,1088265,0.39]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",275495,0.28000000000000003,275549,0.37,228542,0.13]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",212858,0.72,214557,0.74,670905,0.38]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",753053,0.37,754929,0.42,898872,0.46]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",738886,0.42,793414,0.43,1153689,0.36]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",274742,0.3,336000,0.27,231075,0.15]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",212699,0.7,215094,0.72,623616,0.28000000000000003]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",650450,0.39,718202,0.38,597269,0.49]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",598740,0.26,819200,0.33,793414,0.36]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",265054,0.24,264315,0.32,206528,0.16]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",211835,0.67,211809,0.69,578560,0.32]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",563136,0.38,591701,0.39,606208,0.49]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",658495,0.32,638596,0.38,861056,0.31]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",263835,0.24,262272,0.33,204160,0.17]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",208661,0.68,206486,0.7,506368,0.41]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",542057,0.41,551581,0.43,561737,0.52]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1220 (4+4MB)",3,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",654580,0.32,663255,0.35,786746,0.37]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",402372,0.05,388239,0.22,274461,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",696320,0.17,742912,0.19,1162752,0.08]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1376909,0.05,1348309,0.17,2097152,0.02]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1488719,0.05,1591704,0.09,2323623,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",368000,0.05,408461,0.08,252672,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",708096,0.13,688128,0.22,945152,0.11]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",1131762,0.05,808985,0.38,1613885,0.02]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1228294,0.04,1283446,0.08,1758481,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",367744,0.05,419019,0.05,252995,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",464093,0.16,666624,0.24,958976,0.09]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",1148105,0.04,1122304,0.14000000000000001,1619991,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1223768,0.04,1299350,7.0000000000000007E-2,1756299,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",381856,0.04,430848,7.0000000000000007E-2,264384,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",660480,0.11,521076,0.35,805888,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",1025532,0.04,758964,0.34,1160363,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",1101717,0.02,1146680,0.06,1228294,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",333632,0.05,367680,7.0000000000000007E-2,235525,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",589824,0.12,608256,0.15,784384,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",883631,0.03,879240,0.1,1161811,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",668085,0.05,949085,7.0000000000000007E-2,1232855,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",343125,0.02,363200,0.08,236770,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",588800,0.12,497477,0.3,790016,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",852865,0.06,911130,0.06,1152191,0.02]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",935076,0.02,668897,0.34,1232855,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",405317,0.03,448775,0.1,269790,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",727155,0.12,711302,0.21,1155072,0.08]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1409596,0.02,1315622,0.18,2098624,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1479585,0.05,1589734,0.09,2317836,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",376656,0.02,408730,7.0000000000000007E-2,253120,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",704000,0.13,687780,0.21,967680,0.08]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",1144019,0.04,809995,0.37,1613824,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1226782,0.04,1286596,0.08,1758481,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",355456,0.08,410944,0.06,249601,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",428788,0.2,672371,0.23,966656,0.08]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",1153629,0.03,1116811,0.14000000000000001,1611809,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1231331,0.03,1294538,7.0000000000000007E-2,1758481,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",380688,0.04,432576,7.0000000000000007E-2,258432,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",642560,0.13,659456,0.17,805376,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",1048739,0.01,747698,0.34,1158918,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",1093606,0.03,1118907,0.08,1226782,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",338070,0.03,359059,0.09,235525,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",586752,0.12,606473,0.15,790528,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",901834,0.01,872448,0.1,1160363,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",665661,0.05,705032,0.31,1232855,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",338432,0.03,379904,0.04,234786,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",586530,0.12,578560,0.19,778240,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",882529,0.03,667571,0.31,1157720,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",938540,0.02,923715,0.1,1228294,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",402381,0.04,457030,0.08,269884,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",728064,0.12,727552,0.19,1137152,0.09]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1419537,0.02,1393252,0.13,2093056,0.02]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1545812,0,1532433,0.12,2312077,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",377664,0.02,408000,7.0000000000000007E-2,251265,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",689375,0.14000000000000001,556544,0.36,981504,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",1174084,0.01,813071,0.37,1617920,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1243629,0.02,1283446,0.08,1756299,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",357249,7.0000000000000007E-2,404032,0.08,251424,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",460742,0.16,519168,0.4,982016,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",1149539,0.04,796728,0.38,1615900,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1217783,0.04,1286596,0.08,1758481,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",370705,0.06,435840,0.06,260928,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",644096,0.13,635621,0.2,805376,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",1048739,0.01,1051357,0.08,1152191,0.02]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",1118907,0,1128541,7.0000000000000007E-2,1225273,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",342101,0.02,364041,7.0000000000000007E-2,236386,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",583680,0.12,609030,0.15,772608,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",885511,0.03,887722,0.09,1148105,0.02]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",608891,0.1,681314,0.33,1232855,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",336405,0.04,377744,0.04,236386,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",585216,0.12,570277,0.2,777728,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",883631,0.03,656165,0.32,1160363,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",938540,0.02,909545,0.11,1232855,0]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",346420,0.36,348594,0.45,247841,0.25]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",206641,0.79,206001,0.8,711680,0.5]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",731355,0.57999999999999996,750848,0.61,786595,0.65]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",886477,0.53,924838,0.55000000000000004,1100357,0.55000000000000004]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",351964,0.31,382355,0.33,265792,0.15]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",219995,0.77,218187,0.79,821245,0.34]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",808985,0.47,849843,0.49,670905,0.63]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",879240,0.46,837314,0.53,983040,0.5]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",379904,0.25,381744,0.33,272832,0.12]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",219053,0.78,217894,0.79,827392,0.33]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",846813,0.45,864031,0.48,691995,0.62]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",901723,0.45,900617,0.49,1012012,0.48]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",378581,0.24,371904,0.35,271390,0.14000000000000001]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",220049,0.74,218187,0.76,635850,0.31]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",652911,0.42,691995,0.42,614654,0.49]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",771011,0.35,808088,0.36,668897,0.47]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",281308,0.36,378960,0.22,245089,0.15]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",218432,0.71,221502,0.72,652800,0.28999999999999998]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",601360,0.42,601360,0.45,561152,0.54]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",701601,0.36,713758,0.38,782519,0.38]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",282012,0.36,370432,0.24,243200,0.15]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",219236,0.71,218378,0.72,654848,0.28999999999999998]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",614654,0.41,598372,0.45,533906,0.56000000000000005]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",1,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",702456,0.36,747126,0.35,811089,0.36]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",383458,0.28999999999999998,379024,0.4,275997,0.17]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",218835,0.78,218296,0.79,816640,0.43]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",844704,0.52,882529,0.54,951988,0.57999999999999996]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1002030,0.47,1028015,0.5,1251360,0.49]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",385566,0.24,392064,0.32,264637,0.15]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",220451,0.78,221184,0.79,739840,0.4]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",862100,0.44,874358,0.47,888832,0.52]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",906176,0.45,940863,0.47,1116184,0.43]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",384879,0.24,376768,0.34,255712,0.18]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",220424,0.78,221073,0.79,784896,0.37]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",875449,0.43,868352,0.47,878443,0.52]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",902832,0.45,935076,0.47,1100357,0.44]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",386575,0.23,380864,0.34,267806,0.15]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",219264,0.74,221184,0.76,605184,0.34]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",542057,0.36,696931,0.42,608023,0.5]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",780577,0.34,816139,0.35,735281,0.42]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",284188,0.35,378304,0.22,241313,0.16]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",220160,0.71,217975,0.73,605184,0.34]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",618496,0.41,635007,0.42,604696,0.5]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",732601,0.33,745279,0.35,847729,0.33]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",280640,0.36,379520,0.22,244257,0.15]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",218030,0.71,218187,0.72,638976,0.31]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",608782,0.42,625905,0.43,639077,0.48]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",2,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",705895,0.35,774809,0.33,878149,0.3]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",388429,0.28000000000000003,373073,0.41,268446,0.19]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",216546,0.78,218460,0.79,813568,0.43]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",852865,0.51,862958,0.55000000000000004,918156,0.6]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",983833,0.48,994671,0.52,1276356,0.48]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",379800,0.25,373623,0.35,256384,0.18]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",216573,0.78,218460,0.79,748032,0.39]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",846813,0.45,874358,0.47,878443,0.52]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",863157,0.47,981812,0.45,1216296,0.38]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",375057,0.26,375168,0.34,259904,0.16]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",215202,0.78,215525,0.8,681643,0.45]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",822268,0.46,862100,0.48,892928,0.51]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",912626,0.44,949797,0.46,1155102,0.41]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",372677,0.25,373457,0.35,261182,0.17]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",214744,0.75,215417,0.76,653312,0.28999999999999998]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",561152,0.34,719098,0.4,578019,0.52]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",766316,0.35,784470,0.37,689028,0.45]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",277085,0.37,371089,0.24,235973,0.18]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",213450,0.72,215525,0.73,640735,0.3]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",597269,0.43,614654,0.44,620266,0.49]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",699050,0.36,784470,0.32,886477,0.3]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",273474,0.38,372410,0.24,235874,0.18]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",215256,0.71,214610,0.73,630784,0.31]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",592438,0.43,611343,0.44,621039,0.49]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1230 IV (64MB)",3,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",711118,0.35,749914,0.35,851968,0.33]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",508484,0.05,559488,0.11,310976,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",823808,0.19,635392,0.41,1228288,0.09]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1662914,0.04,1615900,0.14000000000000001,2172260,0.02]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1858483,0.01,1025502,0.49,2383127,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",493067,0.02,433821,0.24,295195,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",855552,0.15,835072,0.23,1078784,0.08]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",1487225,0.02,1284538,0.21,1771353,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1294538,0.05,1366010,0.22,1921303,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",479296,0.05,426019,0.25,294747,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",837632,0.17,830976,0.23,1086464,0.08]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",1493173,0.02,918156,0.43,1759081,0.02]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1626203,0,1511750,0.14000000000000001,1921303,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",480579,0.03,499375,0.12,295771,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",743424,0.15,575488,0.38,842752,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",1081344,0.03,1005103,0.15,1183744,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",908419,7.0000000000000007E-2,1056257,0.15,1240532,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",414540,0.05,450880,7.0000000000000007E-2,271774,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",648704,0.16,662016,0.18,840704,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",1012012,0.02,921600,0.15,1190447,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",1074627,0.01,1040770,0.09,1254431,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",423040,0.03,447048,0.08,270016,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",679424,0.12,502875,0.38,845312,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",999770,0.04,1001017,0.08,1190447,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",1061441,0.02,728177,0.36,1254431,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",524352,0.03,569984,0.09,309312,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",826368,0.18,834048,0.23,1245184,0.08]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1701808,0.02,1574991,0.16,2180442,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1858483,0.01,1782190,0.12,2383127,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",495426,0.02,524416,0.08,294454,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",855040,0.15,830976,0.23,1086464,0.08]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",1487225,0.02,883631,0.45,1771353,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1307451,0.04,956729,0.45,1921303,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",478872,0.05,532416,0.06,293787,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",858112,0.15,827904,0.23,1092096,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",1454539,0.04,1413681,0.13,1773230,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1622178,0,1369408,0.22,1916542,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",466611,0.06,428224,0.25,289216,0.08]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",746586,0.15,736256,0.21,836096,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",1103162,0.01,933342,0.21,1183744,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",939700,0.04,1143901,0.08,1240532,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",424384,0.03,442173,0.09,270464,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",678575,0.12,518144,0.36,836096,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",998176,0.04,999424,0.08,1190447,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",1060141,0.02,727299,0.36,1254431,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",425482,0.03,423896,0.12,270302,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",666112,0.13,674816,0.17,839118,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",1010448,0.02,897024,0.17,1190447,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",1054969,0.03,1062745,7.0000000000000007E-2,1254431,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",515520,0.04,572416,0.09,309106,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",859136,0.15,813056,0.25,1233920,0.09]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1699840,0.02,1599536,0.15,2172260,0.02]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1816839,0.03,1803447,0.11,2383127,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",484578,0.04,502208,0.12,291520,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",800256,0.2,613376,0.43,1096704,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",1452264,0.04,1406666,0.14000000000000001,1769472,0.02]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1242078,0.08,1543915,0.12,1921303,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",482944,0.04,504849,0.11,295286,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",856064,0.15,803367,0.25,1089024,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",1448173,0.04,1439992,0.11,1773568,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1608245,0.01,943198,0.46,1921303,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",485632,0.02,521792,0.09,296960,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",758272,0.13,734720,0.21,840704,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",1084084,0.03,1050046,0.11,1182266,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",942029,0.04,1139756,0.08,1240532,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",422859,0.03,448192,7.0000000000000007E-2,267102,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",678912,0.12,518144,0.36,843264,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",999770,0.03,1001017,0.08,1190447,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",1056257,0.03,718630,0.37,1254431,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",425162,0.03,436352,0.1,267870,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",659968,0.14000000000000001,677376,0.16,840704,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",1015808,0.02,967125,0.11,1190447,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",1081662,0,1045961,0.08,1254431,0]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",377854,0.36,364864,0.46,260608,0.19]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",211403,0.77,211703,0.78,781824,0.37]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",779413,0.54,821242,0.53,809995,0.55000000000000004]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",953250,0.47,999565,0.47,1235914,0.36]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",367552,0.33,364160,0.41,245985,0.2]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",209933,0.77,205004,0.79,704512,0.36]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",710041,0.52,704512,0.54,764995,0.51]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",864210,0.45,906176,0.45,1004507,0.4]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",354874,0.35,352832,0.43,240673,0.22]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",206946,0.78,205924,0.79,706560,0.36]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",715905,0.51,699541,0.54,772213,0.51]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",848785,0.46,892947,0.45,1026757,0.38]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",386191,0.27,381616,0.35,255296,0.17]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",219154,0.72,218296,0.74,653824,0.3]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",642269,0.37,624346,0.4,632508,0.48]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",611133,0.36,730825,0.33,793414,0.37]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",281096,0.37,381968,0.22,229316,0.16]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",219401,0.68,218296,0.69,535552,0.31]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",581632,0.36,576814,0.38,555666,0.43]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",637044,0.33,661661,0.31,719996,0.28999999999999998]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",280604,0.31,279232,0.37,221576,0.14000000000000001]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",220049,0.63,221585,0.64,522610,0.21]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",507904,0.33,542057,0.28999999999999998,471833,0.41]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",571258,0.27,561737,0.28999999999999998,617957,0.25]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",384191,0.35,374303,0.44,271582,0.16]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",219483,0.76,218378,0.78,782336,0.37]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",822268,0.51,841671,0.52,766216,0.56999999999999995]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",967321,0.47,1013274,0.46,1145448,0.4]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",389212,0.28999999999999998,381312,0.38,259583,0.16]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",218542,0.76,221474,0.77,771584,0.3]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",790528,0.46,795735,0.48,693718,0.55000000000000004]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",892947,0.44,955567,0.42,1023000,0.38]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",388895,0.28999999999999998,381729,0.38,256415,0.17]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",219026,0.76,217894,0.77,757760,0.31]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",783493,0.47,835502,0.45,844704,0.46]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",911531,0.42,949085,0.42,1070637,0.36]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",398080,0.25,391582,0.34,251969,0.18]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",219428,0.72,220714,0.73,602653,0.35]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",556360,0.38,639077,0.39,652099,0.46]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",699899,0.35,714642,0.35,831188,0.34]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",283456,0.37,382224,0.22,231651,0.15]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",219857,0.67,218378,0.69,599826,0.23]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",603943,0.33,591701,0.36,595781,0.39]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",665661,0.3,676292,0.3,746201,0.27]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",284060,0.3,280049,0.36,221156,0.14000000000000001]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",219026,0.63,217894,0.64,491335,0.25]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",537982,0.28999999999999998,567924,0.26,515451,0.35]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",578968,0.26,576140,0.27,648871,0.21]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",393166,0.34,386588,0.43,265182,0.18]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",220341,0.76,221640,0.77,784427,0.37]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",867267,0.48,897024,0.49,877349,0.51]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1020511,0.44,1016800,0.46,1116184,0.42]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",391104,0.28999999999999998,381171,0.38,249153,0.19]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",217491,0.77,218460,0.77,710144,0.35]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",830449,0.44,784470,0.48,844704,0.46]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",906176,0.43,952096,0.42,1064053,0.36]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",391439,0.28999999999999998,373333,0.39,253568,0.18]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",216627,0.77,218542,0.77,711814,0.35]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",821242,0.44,801813,0.47,793631,0.49]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",910673,0.42,974513,0.41,1090929,0.34]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",387919,0.27,382930,0.35,252480,0.18]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",216816,0.73,218057,0.74,690848,0.26]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",550208,0.39,630784,0.4,629996,0.48]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",703313,0.34,722939,0.34,835262,0.34]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",280284,0.37,382544,0.22,231907,0.15]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",218030,0.68,215848,0.69,540508,0.3]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",572009,0.37,599862,0.35,603192,0.38]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",653725,0.31,668085,0.31,735281,0.28000000000000003]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",274909,0.32,280206,0.36,216056,0.16]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",215094,0.63,215068,0.64,490762,0.26]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",536576,0.28999999999999998,580905,0.24,559055,0.3]
["PFS3_18.5_020/030","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",576844,0.26,583262,0.27,622592,0.24]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",569152,0.03,597120,0.1,304601,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",811008,0.16,793600,0.22,1095168,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1624081,0.02,1450453,0.16,1740800,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1728063,0.03,1667000,0.1,1877080,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",511296,0.06,545430,0.1,285184,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",829952,0.14000000000000001,578048,0.43,997376,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",1393252,0.04,1347355,0.1,1511740,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1369408,0.05,1409024,0.13,1630248,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",525248,0.03,554048,0.08,287836,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",803328,0.16,786944,0.22,989696,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",1378628,0.05,1309083,0.13,1509537,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1517335,0.03,942029,0.41,1630248,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",516608,0.02,434854,0.25,287032,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",719872,0.12,673792,0.21,849920,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",991232,0.02,949085,0.08,1179648,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",954931,0.03,710242,0.34,1238989,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",426762,0.04,460576,0.05,258559,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",591872,0.14000000000000001,606985,0.15,716927,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",841671,0.06,858014,0.06,954883,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",905059,0.03,853786,0.11,1002030,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",397888,0.01,349184,0.2,244193,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",542720,0.09,522610,0.15,616448,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",733184,0.02,554284,0.27,784470,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",771011,0.01,574037,0.27,816139,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",561920,0.04,585920,0.11,305369,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",810496,0.17,613888,0.39,1100800,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1593456,0.04,1507328,0.12,1738626,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1708933,0.04,1656672,0.11,1877080,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",518976,0.04,551055,0.09,284416,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",791040,0.18,809472,0.2,994304,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",1409596,0.03,1317265,0.12,1513627,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1367707,0.05,1431059,0.11,1630248,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",526272,0.03,559424,0.08,284330,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",807424,0.16,782564,0.22,995840,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",1429504,0.02,1315622,0.12,1511740,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1553445,0,1431059,0.11,1630248,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",505600,0.04,530368,0.09,288347,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",720384,0.12,684200,0.19,847360,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",982224,0.03,691359,0.33,1183744,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",879677,0.11,738886,0.32,1242078,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",425888,0.04,459718,0.05,254432,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",591133,0.14000000000000001,601088,0.16,714240,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",861027,0.04,615153,0.33,956073,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",910673,0.03,663255,0.3,1002030,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",390144,0.03,360192,0.17,245120,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",542553,0.09,518144,0.16,618496,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",737280,0.01,550894,0.27,784470,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",752723,0.03,717309,0.09,816139,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",573171,0.02,599762,0.09,301914,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",835072,0.14000000000000001,595968,0.41,1099776,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1593456,0.04,1481293,0.14000000000000001,1742717,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1689155,0.05,1628223,0.12,1877080,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",500288,0.08,549696,0.09,285880,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",809472,0.16,803328,0.21,990720,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",1394992,0.04,1287022,0.14000000000000001,1513627,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1283446,0.11,1400272,0.13,1630248,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",509634,0.06,548498,0.09,286748,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",786432,0.18,795648,0.21,990720,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",1370446,0.06,1348309,0.1,1513627,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1528631,0.02,1438196,0.11,1630248,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",506560,0.03,527936,0.09,286812,7.0000000000000007E-2]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",720384,0.12,518961,0.39,850432,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",1001017,0.01,957267,0.08,1179648,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",1045961,0.01,1012012,7.0000000000000007E-2,1240532,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",372864,0.09,460614,0.05,258816,0.06]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",589599,0.15,606720,0.15,716416,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",871358,0.03,622795,0.32,954883,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",916358,0.02,658495,0.31,1002030,0]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",387694,0.04,360402,0.17,244544,0.05]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",543744,0.09,521076,0.15,617723,0.04]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",736359,0.01,550894,0.27,782519,0.01]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",737079,0.05,744359,0.06,816139,0]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",384558,0.36,374384,0.45,267261,0.17]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",217491,0.77,218323,0.78,781359,0.37]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",813071,0.52,826359,0.53,736771,0.59]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",956729,0.47,960234,0.49,1110779,0.42]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",387125,0.3,373397,0.4,255648,0.16]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",219510,0.77,217894,0.78,743518,0.33]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",790670,0.46,789541,0.48,640669,0.59]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",896218,0.43,900617,0.45,1042063,0.37]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",384591,0.3,368960,0.4,256255,0.16]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",218889,0.77,218835,0.78,808448,0.27]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",771251,0.48,821242,0.46,754929,0.52]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",881430,0.44,923715,0.44,1044658,0.37]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",385984,0.28000000000000003,378087,0.36,250496,0.18]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",218569,0.73,220644,0.73,652800,0.3]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",547465,0.39,605451,0.42,609826,0.5]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",691506,0.35,714642,0.35,811089,0.36]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",279023,0.38,380160,0.23,231064,0.15]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",218378,0.68,218378,0.69,576000,0.26]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",558360,0.38,599862,0.35,564542,0.42]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",649675,0.31,682159,0.28999999999999998,714642,0.3]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",274504,0.32,278484,0.37,216292,0.16]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",218323,0.63,216952,0.64,500224,0.24]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",522329,0.31,559055,0.27,527066,0.34]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",561737,0.28000000000000003,581107,0.27,641723,0.22]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",390784,0.34,382915,0.43,273117,0.15]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",218432,0.77,217975,0.78,775168,0.37]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",823296,0.51,877061,0.5,799816,0.56000000000000005]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",944369,0.48,1025502,0.46,1100357,0.43]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",394368,0.28000000000000003,388856,0.37,251776,0.17]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",217975,0.77,221557,0.77,827904,0.25]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",853929,0.42,789541,0.48,828381,0.47]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",899513,0.43,924838,0.43,1035630,0.38]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",394958,0.28000000000000003,388608,0.37,251712,0.17]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",219373,0.77,215740,0.78,747520,0.32]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",849691,0.42,837586,0.45,908176,0.42]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",892947,0.44,935076,0.43,1067994,0.36]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",394560,0.26,378459,0.36,244226,0.2]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",216467,0.73,217975,0.74,697344,0.25]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",542057,0.4,628427,0.4,635007,0.48]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",698204,0.35,673809,0.38,803137,0.36]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",279597,0.38,379920,0.23,234658,0.14000000000000001]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",217866,0.68,218084,0.69,548352,0.28999999999999998]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",582089,0.36,601360,0.35,597269,0.39]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",644880,0.32,674635,0.3,724676,0.28999999999999998]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",278807,0.31,278842,0.37,217700,0.15]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",217006,0.63,214447,0.64,461535,0.3]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",542057,0.28000000000000003,560451,0.27,524450,0.34]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",577551,0.26,606666,0.24,683005,0.17]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",387246,0.35,382244,0.43,269470,0.16]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",218187,0.77,218542,0.78,716288,0.42]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",840623,0.5,838631,0.52,814086,0.55000000000000004]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",992242,0.45,1035630,0.45,1187188,0.38]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",389260,0.28999999999999998,382642,0.38,252352,0.17]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",218084,0.77,217997,0.78,679424,0.38]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",773177,0.47,792642,0.48,815104,0.48]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",896218,0.43,894035,0.45,974513,0.41]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",375500,0.32,361186,0.42,255520,0.16]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",213935,0.77,215068,0.78,655053,0.41]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",787574,0.46,769086,0.49,785617,0.5]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",889700,0.44,911805,0.44,1061441,0.36]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",379689,0.28999999999999998,373885,0.37,258463,0.15]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",214878,0.73,214610,0.74,650450,0.3]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",542732,0.4,626688,0.4,637382,0.47]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",699050,0.35,694839,0.36,828158,0.34]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",276736,0.38,366188,0.26,228195,0.16]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",212832,0.69,214153,0.69,524800,0.32]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",567924,0.37,579459,0.37,607267,0.38]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",645674,0.32,664055,0.31,711996,0.3]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",274368,0.33,272385,0.38,217620,0.15]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",213962,0.64,212400,0.65,490312,0.26]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",527724,0.3,529830,0.31,550894,0.31]
["PFS3_18.5_040","Samsung 356 MB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",570567,0.27,576140,0.27,661661,0.2]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",566208,0.04,582976,0.13,303002,0.06]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",817152,0.16,808448,0.2,1104896,7.0000000000000007E-2]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1603627,0.03,1495397,0.13,1738626,0.01]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1773421,0.01,1634314,0.12,1877080,0]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",530560,0.03,557056,0.09,290944,0.06]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",818688,0.16,600576,0.41,996352,0.06]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",1393252,0.04,1347584,0.1,1511424,0.01]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1333486,0.08,919247,0.43,1630248,0]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",536256,0.02,536064,0.12,286456,7.0000000000000007E-2]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",816128,0.16,811520,0.2,990720,0.06]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",1427719,0.02,1319708,0.12,1511424,0.01]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1536255,0.02,1359265,0.16,1630248,0]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",503360,0.05,539712,0.08,284444,7.0000000000000007E-2]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",704000,0.14000000000000001,677553,0.21,846848,0.06]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",995690,0.02,958464,7.0000000000000007E-2,1179321,0.01]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",927678,0.06,975722,0.1,1242078,0]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",422987,0.05,452878,7.0000000000000007E-2,259647,0.06]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",620544,0.1,578860,0.19,718336,0.04]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",870272,0.03,640669,0.3,954368,0.01]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",888623,0.05,648871,0.32,1002030,0]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",393294,0.03,395737,0.1,244418,0.05]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",531456,0.11,530792,0.14000000000000001,618235,0.04]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",740450,0.01,684032,0.1,783493,0.01]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",757094,0.02,732601,7.0000000000000007E-2,816139,0]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",556544,0.06,594034,0.11,302772,0.06]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",833536,0.14000000000000001,753152,0.26,1098240,7.0000000000000007E-2]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1595445,0.04,1515520,0.12,1738626,0.01]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1743322,0.02,968512,0.47,1877080,0]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",522432,0.04,463168,0.24,288704,0.06]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",798720,0.18,795136,0.22,988672,0.06]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",1423628,0.02,1319708,0.12,1511740,0.01]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1366010,0.06,1330186,0.17,1630248,0]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",526382,0.04,571381,0.06,290011,0.06]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",829952,0.15,577536,0.43,988160,0.06]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",1393252,0.04,1349992,0.1,1511740,0.01]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1549619,0.01,1449199,0.1,1630248,0]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",509376,0.04,526528,0.11,286556,7.0000000000000007E-2]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",722432,0.12,689152,0.19,847872,0.06]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",978944,0.03,685557,0.34,1180792,0.01]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",950272,0.04,959063,0.11,1242078,0]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",430716,0.03,464448,0.05,257311,0.06]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",606985,0.12,591872,0.17,716288,0.05]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",883631,0.01,797722,0.13,951988,0.01]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",914076,0.03,862105,0.1,1002030,0]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",372927,0.08,411596,0.06,245601,0.05]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",524288,0.13,523776,0.15,620032,0.04]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",726364,0.03,544087,0.28000000000000003,784470,0.01]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",758006,0.02,568505,0.28000000000000003,816139,0]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",565504,0.04,595072,0.11,305177,0.06]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",814080,0.16,605696,0.4,1102336,7.0000000000000007E-2]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1587263,0.04,1400832,0.19,1734535,0.01]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1706834,0.04,1656672,0.1,1877080,0]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",524464,0.04,561344,0.08,290231,0.06]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",813568,0.16,600064,0.41,988672,0.06]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",1399083,0.03,1345901,0.1,1507654,0.01]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1326901,0.08,928226,0.42,1630248,0]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",531200,0.02,531776,0.12,287388,0.06]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",820736,0.16,815616,0.2,980480,7.0000000000000007E-2]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",1366356,0.06,1350710,0.1,1505446,0.01]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1522962,0.03,1443877,0.1,1630248,0]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",514176,0.03,529280,0.1,287772,0.06]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",721920,0.12,641536,0.25,851456,0.05]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",992845,0.02,698669,0.32,1179321,0.01]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",948937,0.04,717309,0.34,1242078,0]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",430602,0.04,459968,0.05,258399,0.06]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",604672,0.13,570277,0.2,718336,0.05]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",840623,0.06,856946,0.06,953176,0.01]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",922594,0.02,649675,0.32,1002030,0]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",400361,0.01,402358,0.08,245376,0.05]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",532837,0.11,531968,0.14000000000000001,620032,0.03]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",740450,0.01,664326,0.12,783493,0.01]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",757094,0.02,715529,0.09,816139,0]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",389824,"n/a",388495,"n/a",306176,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",218780,"n/a",218269,"n/a",867840,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",969540,"n/a",980588,"n/a",953176,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1396801,"n/a",1381396,"n/a",1304199,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",388767,"n/a",390906,"n/a",307776,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",218542,"n/a",218323,"n/a",823290,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",964245,"n/a",924540,"n/a",918156,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1219274,"n/a",1299350,"n/a",1310720,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",385310,"n/a",391544,"n/a",307225,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",220479,"n/a",217328,"n/a",823296,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",968331,"n/a",957267,"n/a",976502,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1128541,"n/a",1206384,"n/a",1297742,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",385918,"n/a",387770,"n/a",294555,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",219455,"n/a",217894,"n/a",602142,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",671744,"n/a",678240,"n/a",683178,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",940863,"n/a",966132,"n/a",921475,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",391732,"n/a",377280,"n/a",257119,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",217274,"n/a",216576,"n/a",621814,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",656175,"n/a",681476,"n/a",683178,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",839377,"n/a",855851,"n/a",925965,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",310080,"n/a",376576,"n/a",256384,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",217812,"n/a",217409,"n/a",601360,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",632508,"n/a",644750,"n/a",654546,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",1,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",719996,"n/a",729058,"n/a",785450,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",394368,"n/a",388736,"n/a",313048,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",218644,"n/a",221529,"n/a",784981,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",983448,"n/a",984674,"n/a",984674,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1483225,"n/a",1519206,"n/a",1566987,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",395008,"n/a",388160,"n/a",307353,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",219081,"n/a",217033,"n/a",784896,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",996931,"n/a",974848,"n/a",983448,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1309083,"n/a",1274765,"n/a",1312320,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",387776,"n/a",378176,"n/a",289085,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",216170,"n/a",218514,"n/a",717950,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",954368,"n/a",961358,"n/a",983040,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1152281,"n/a",1285019,"n/a",1312320,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",387456,"n/a",382724,"n/a",289883,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",217464,"n/a",217975,"n/a",561664,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",680628,"n/a",707723,"n/a",682326,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",962585,"n/a",981812,"n/a",983040,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",387997,"n/a",373345,"n/a",261279,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",217921,"n/a",218542,"n/a",598016,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",640669,"n/a",655360,"n/a",656992,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",850904,"n/a",871661,"n/a",921475,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",297653,"n/a",371177,"n/a",245281,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",214584,"n/a",215417,"n/a",523264,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",595040,"n/a",595040,"n/a",620266,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",2,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",695677,"n/a",714642,"n/a",743441,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",381159,"n/a",373689,"n/a",290203,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",215390,"n/a",215417,"n/a",923517,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",914076,"n/a",923387,"n/a",924540,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1384790,"n/a",1425752,"n/a",1389912,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",382914,"n/a",373160,"n/a",295259,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",215390,"n/a",215068,"n/a",741888,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",899995,"n/a",924540,"n/a",923387,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1274765,"n/a",1310720,"n/a",1309083,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",380470,"n/a",372805,"n/a",295259,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",215417,"n/a",215525,"n/a",740864,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",858014,"n/a",848785,"n/a",872183,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1035630,"n/a",1141174,"n/a",1129931,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",369141,"n/a",362230,"n/a",299418,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",210706,"n/a",211782,"n/a",559940,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",778443,"n/a",781547,"n/a",713233,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",942029,"n/a",978149,"n/a",983040,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",354963,"n/a",340864,"n/a",264414,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",203854,"n/a",206796,"n/a",516341,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",544778,"n/a",546813,"n/a",561737,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",694003,"n/a",719098,"n/a",749914,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",275172,"n/a",341674,"n/a",233698,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",209631,"n/a",217812,"n/a",531303,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",585728,"n/a",605451,"n/a",626088,"n/a"]
["PFS3_18.5_060","Samsung 356 MB","Blizzard 1260 (128MB)",3,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",691506,"n/a",683853,"n/a",749914,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",669120,"n/a",534784,"n/a",350484,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",915456,"n/a",648704,"n/a",1309696,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1656808,"n/a",1534082,"n/a",1955443,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1830431,"n/a",1680824,"n/a",2111444,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",617723,"n/a",653888,"n/a",336277,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",888320,"n/a",878592,"n/a",1176064,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",1468628,"n/a",1340137,"n/a",1685445,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1434618,"n/a",1465401,"n/a",1810118,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",624000,"n/a",625856,"n/a",336448,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",911872,"n/a",861696,"n/a",1174016,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",1482752,"n/a",1276356,"n/a",1687552,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1576080,"n/a",1497965,"n/a",1810118,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",579584,"n/a",493138,"n/a",328086,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",737280,"n/a",767488,"n/a",829440,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",903543,"n/a",923387,"n/a",1092266,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",1052402,"n/a",1044658,"n/a",1135524,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",500736,"n/a",507520,"n/a",296602,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",670720,"n/a",642269,"n/a",827904,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",918156,"n/a",618187,"n/a",1043176,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",961408,"n/a",902832,"n/a",1090929,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",453383,"n/a",396096,"n/a",279389,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",571190,"n/a",568832,"n/a",702609,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",741763,"n/a",707723,"n/a",852865,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",786746,"n/a",757094,"n/a",885407,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",667456,"n/a",544576,"n/a",350740,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",896000,"n/a",660480,"n/a",1311232,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1695744,"n/a",998176,"n/a",1959534,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1695458,"n/a",1708933,"n/a",2111444,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",633000,"n/a",659136,"n/a",336192,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",888832,"n/a",876032,"n/a",1174016,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",1454539,"n/a",1349030,"n/a",1685445,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1439992,"n/a",1454559,"n/a",1810118,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",619776,"n/a",631274,"n/a",337109,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",911872,"n/a",855552,"n/a",1174016,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",1470464,"n/a",1347584,"n/a",1685445,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1597643,"n/a",927094,"n/a",1810118,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",588352,"n/a",592960,"n/a",327191,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",786944,"n/a",756224,"n/a",828928,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",944627,"n/a",964245,"n/a",1090904,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",1070637,"n/a",1020511,"n/a",1135524,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",506304,"n/a",513728,"n/a",297397,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",657408,"n/a",517044,"n/a",829952,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",918156,"n/a",820220,"n/a",1041875,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",953250,"n/a",900617,"n/a",1090929,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",445312,"n/a",440181,"n/a",279069,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",574976,"n/a",561474,"n/a",703121,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",762141,"n/a",719996,"n/a",852865,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",793414,"n/a",567820,"n/a",885407,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 512 byte, MEMF_FAST, LONG-aligned buffer.",512,"MEMF_FAST","LONG",676224,"n/a",690688,"n/a",348436,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 4096 byte, MEMF_FAST, LONG-aligned buffer.",4096,"MEMF_FAST","LONG",911360,"n/a",864768,"n/a",1308160,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 32768 byte, MEMF_FAST, LONG-aligned buffer.",32768,"MEMF_FAST","LONG",1679257,"n/a",1531904,"n/a",1957888,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 262144 byte, MEMF_FAST, LONG-aligned buffer.",262144,"MEMF_FAST","LONG",1828152,"n/a",1632278,"n/a",2111444,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 512 byte, MEMF_FAST, WORD-aligned buffer.",512,"MEMF_FAST","WORD",643904,"n/a",660928,"n/a",336448,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 4096 byte, MEMF_FAST, WORD-aligned buffer.",4096,"MEMF_FAST","WORD",891904,"n/a",879104,"n/a",1174016,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 32768 byte, MEMF_FAST, WORD-aligned buffer.",32768,"MEMF_FAST","WORD",1468628,"n/a",1350710,"n/a",1685445,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 262144 byte, MEMF_FAST, WORD-aligned buffer.",262144,"MEMF_FAST","WORD",1413521,"n/a",1384790,"n/a",1810118,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 512 byte, MEMF_FAST, BYTE-aligned buffer.",512,"MEMF_FAST","BYTE",603533,"n/a",526784,"n/a",338901,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 4096 byte, MEMF_FAST, BYTE-aligned buffer.",4096,"MEMF_FAST","BYTE",897536,"n/a",651545,"n/a",1175040,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 32768 byte, MEMF_FAST, BYTE-aligned buffer.",32768,"MEMF_FAST","BYTE",1442282,"n/a",1264083,"n/a",1687552,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 262144 byte, MEMF_FAST, BYTE-aligned buffer.",262144,"MEMF_FAST","BYTE",1576080,"n/a",1503569,"n/a",1810118,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 512 byte, MEMF_CHIP, LONG-aligned buffer.",512,"MEMF_CHIP","LONG",561024,"n/a",507264,"n/a",327959,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 4096 byte, MEMF_CHIP, LONG-aligned buffer.",4096,"MEMF_CHIP","LONG",762368,"n/a",592896,"n/a",829440,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 32768 byte, MEMF_CHIP, LONG-aligned buffer.",32768,"MEMF_CHIP","LONG",905914,"n/a",715012,"n/a",1090904,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 262144 byte, MEMF_CHIP, LONG-aligned buffer.",262144,"MEMF_CHIP","LONG",1031809,"n/a",735281,"n/a",1135524,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 512 byte, MEMF_CHIP, WORD-aligned buffer.",512,"MEMF_CHIP","WORD",497920,"n/a",417960,"n/a",299072,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 4096 byte, MEMF_CHIP, WORD-aligned buffer.",4096,"MEMF_CHIP","WORD",670720,"n/a",610816,"n/a",828416,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 32768 byte, MEMF_CHIP, WORD-aligned buffer.",32768,"MEMF_CHIP","WORD",897753,"n/a",835584,"n/a",1041875,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 262144 byte, MEMF_CHIP, WORD-aligned buffer.",262144,"MEMF_CHIP","WORD",916358,"n/a",873813,"n/a",1090929,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 512 byte, MEMF_CHIP, BYTE-aligned buffer.",512,"MEMF_CHIP","BYTE",435456,"n/a",465920,"n/a",279197,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 4096 byte, MEMF_CHIP, BYTE-aligned buffer.",4096,"MEMF_CHIP","BYTE",576000,"n/a",537088,"n/a",704000,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 32768 byte, MEMF_CHIP, BYTE-aligned buffer.",32768,"MEMF_CHIP","BYTE",744541,"n/a",568633,"n/a",852865,"n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,"Testing with a 262144 byte, MEMF_CHIP, BYTE-aligned buffer.",262144,"MEMF_CHIP","BYTE",778645,"n/a",601538,"n/a",884341,"n/a"]

{"sheet":"KT_Adresáře","index":6,"n_rows":13,"n_cols":5,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
[]
["File System","(Vše)"]
[]
[null,"Popisky sloupců"]
[null,"Samsung 356MB",null,"Sandisk CF 4GB"]
["Popisky řádků","Průměr z Seek/Read (seeks/sec)","Průměr z Seek/Read (seeks/sec)2","Průměr z Seek/Read (seeks/sec)","Průměr z Seek/Read (seeks/sec)2"]
["Amiga 1200 (no FAST]",200.33333333333334,0.535650623885918,333.66666666666669,0.33943709732112581]
["MemoryMaster1200(9MB)",299,0.79946524064171121,602.33333333333337,0.61275008477449988]
["Blizzard 1200 (4MB)",279,0.74598930481283421,606,0.61648016276703965]
["Blizzard 1220 (4+4MB)",361,0.96524064171122992,808.66666666666663,0.82265174635469651]
["Blizzard 1230 IV (64MB)",374,1,983,1]
["Blizzard 1240 (64MB)",413.83333333333331,1.10650623885918,1091,1.1098677517802644]
["Blizzard 1260 (128MB)",472.33333333333331,1.2629233511586453,1275.6666666666667,1.297728043404544]

{"sheet":"TestManipulaceSAdresáři","index":7,"n_rows":49,"n_cols":17,"rows_kept":49,"cut":false,"hidden":false,"merged":[]}
["File System","Disk","Accelerator","Test #","File Create in files/sec","CPU Available","File Open in files/sec","CPU Available2","Directory Scan in files/sec","CPU Available3","File Delete in files/sec","CPU Available4","Seek/Read (seeks/sec)","CPU Available5","CPU Speed Rating","Average CPU Available","CPU Availability Index"]
["PFS3_18.5_020/030","Samsung 356MB","Amiga 1200 (no FAST]",1,77,0.02,101,0,652,0,86,0.02,200,0.39,432,0.26,112]
["PFS3_18.5_020/030","Samsung 356MB","Amiga 1200 (no FAST]",2,79,0.01,102,0,653,0,88,0,201,0.38,432,0.26,112]
["PFS3_18.5_020/030","Samsung 356MB","Amiga 1200 (no FAST]",3,79,0.01,102,0,653,0,87,0.01,200,0.38,432,0.25,108]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",1,78,0,99,0,651,0,88,0.01,334,0,432,0.04,17]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",2,79,0,101,0,651,0,87,0.01,334,0.01,432,0.05,22]
["PFS3_18.5_020/030","Sandisk CF 4GB","Amiga 1200 (no FAST]",3,79,0,101,0,651,0,87,0.01,333,0.01,432,0.05,22]
["PFS3_18.5_020/030","Samsung 356MB","MemoryMaster1200(9MB)",1,127,0.03,166,0,1110,0,151,0.01,302,0.49,633,0.36,228]
["PFS3_18.5_020/030","Samsung 356MB","MemoryMaster1200(9MB)",2,127,0.03,167,0,1110,0,148,0.02,300,0.49,633,0.35,222]
["PFS3_18.5_020/030","Samsung 356MB","MemoryMaster1200(9MB)",3,127,0.03,167,0,1111,0,149,0.01,295,0.49,633,0.37,234]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",1,135,0,175,0,1108,0,153,0,603,0.01,633,7.0000000000000007E-2,44]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",2,135,0,175,0,1108,0,153,0,602,0.01,633,7.0000000000000007E-2,44]
["PFS3_18.5_020/030","Sandisk CF 4GB","MemoryMaster1200(9MB)",3,135,0,174,0,1108,0,153,0,602,0.01,633,7.0000000000000007E-2,44]
["PFS3_18.5_020/030","Samsung 356MB","Blizzard 1200 (4MB)",1,132,0.03,175,0,1116,0,151,0.02,287,0.51,635,0.35,222]
["PFS3_18.5_020/030","Samsung 356MB","Blizzard 1200 (4MB)",2,131,0.03,175,0,1115,0,151,0.01,298,0.49,635,0.36,229]
["PFS3_18.5_020/030","Samsung 356MB","Blizzard 1200 (4MB)",3,131,0.03,175,0,1116,0,150,0.02,252,0.56000000000000005,635,0.38,241]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",1,136,0,176,0,1113,0,154,0,607,0,635,0.06,38]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",2,135,0,176,0,1113,0,154,0,605,0.01,635,7.0000000000000007E-2,44]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1200 (4MB)",3,136,0,176,0,1114,0,154,0,606,0.01,635,0.06,38]
["PFS3_18.5_020/030","Samsung 356MB","Blizzard 1220 (4+4MB)",1,205,0.05,282,0,1606,0,250,0.02,392,0.53,1169,0.4,468]
["PFS3_18.5_020/030","Samsung 356MB","Blizzard 1220 (4+4MB)",2,203,0.04,277,0,1541,0,244,0.03,374,0.54,1166,0.39,455]
["PFS3_18.5_020/030","Samsung 356MB","Blizzard 1220 (4+4MB)",3,202,0.04,276,0,1522,0,250,0.01,317,0.6,1167,0.4,467]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",1,214,0,279,0,1578,0,258,0,820,0.01,1167,0.08,93]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",2,211,0,277,0,1551,0,252,0,805,0.01,1167,0.08,93]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1220 (4+4MB)",3,212,0,277,0,1547,0,252,0,801,0.01,1167,0.08,93]
["PFS3_18.5_020/030","Samsung 356MB","Blizzard 1230 IV (64MB)",1,298,7.0000000000000007E-2,410,0,2062,0,375,0.03,367,0.63,2740,0.44,1206]
["PFS3_18.5_020/030","Samsung 356MB","Blizzard 1230 IV (64MB)",2,297,7.0000000000000007E-2,410,0,2061,0,372,0.04,386,0.61,2737,0.42,1150]
["PFS3_18.5_020/030","Samsung 356MB","Blizzard 1230 IV (64MB)",3,302,0.06,412,0,2061,0,374,0.04,369,0.63,2741,0.42,1151]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",1,321,0,413,0,2060,0,388,0,987,0.01,2738,0.1,274]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",2,321,0,413,0,2059,0,388,0,975,0.03,2741,0.09,247]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1230 IV (64MB)",3,321,0,413,0,2059,0,388,0,987,0.01,2739,0.08,219]
["PFS3_18.5_020/030","Samsung 356MB","Blizzard 1240 (64MB)",1,372,0.1,550,0,2423,0,526,0.05,428,0.61,4933,0.41,2023]
["PFS3_18.5_020/030","Samsung 356MB","Blizzard 1240 (64MB)",2,378,0.09,549,0,2423,0,530,0.04,405,0.63,4942,0.39,1927]
["PFS3_18.5_020/030","Samsung 356MB","Blizzard 1240 (64MB)",3,374,0.09,550,0,2423,0,524,0.05,422,0.61,4941,0.39,1927]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,409,0,543,0,2399,0,549,0,1085,0.02,4933,0.08,395]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,411,0,543,0,2398,0,549,0,1081,0.02,4931,0.08,395]
["PFS3_18.5_020/030","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,411,0,543,0,2399,0,549,0,1083,0.02,4932,0.08,395]
["PFS3_18.5_040","Samsung 356MB","Blizzard 1240 (64MB)",1,383,0.09,553,0,2442,0,556,0.04,405,0.63,4932,0.4,1973]
["PFS3_18.5_040","Samsung 356MB","Blizzard 1240 (64MB)",2,381,0.09,550,0,2446,0,554,0.01,432,0.6,4942,0.39,1927]
["PFS3_18.5_040","Samsung 356MB","Blizzard 1240 (64MB)",3,386,7.0000000000000007E-2,551,0,2445,0,533,0.05,391,0.64,4941,0.4,1976]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",1,433,0,583,0,2433,0,578,0,1099,0.02,4935,0.08,395]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",2,435,0,582,0,2436,0,570,0,1100,0.02,4932,0.09,444]
["PFS3_18.5_040","Sandisk CF 4GB","Blizzard 1240 (64MB)",3,436,0,583,0,2436,0,571,0,1098,0.02,4932,0.09,444]
["PFS3_18.5_060","Samsung 356MB","Blizzard 1260 (128MB)",1,507,"n/a",777,"n/a",3032,"n/a",791,"n/a",434,"n/a","n/a","n/a","n/a"]
["PFS3_18.5_060","Samsung 356MB","Blizzard 1260 (128MB)",2,509,"n/a",773,"n/a",3041,"n/a",744,"n/a",487,"n/a","n/a","n/a","n/a"]
["PFS3_18.5_060","Samsung 356MB","Blizzard 1260 (128MB)",3,503,"n/a",773,"n/a",3041,"n/a",718,"n/a",496,"n/a","n/a","n/a","n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",1,569,"n/a",774,"n/a",3019,"n/a",804,"n/a",1273,"n/a","n/a","n/a","n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",2,568,"n/a",770,"n/a",3027,"n/a",789,"n/a",1277,"n/a","n/a","n/a","n/a"]
["PFS3_18.5_060","Sandisk CF 4GB","Blizzard 1260 (128MB)",3,564,"n/a",771,"n/a",3026,"n/a",790,"n/a",1277,"n/a","n/a","n/a","n/a"]